For 1990-2009 cars

# INTERMITTENT OR IN-OPERATIVE CENTER HIGH MOUNTED STOP LAMP

1988 FIRENZA STYLE 37, CUTLASS CIERA STYLE 37

If an intermittent or in-operative center high mounted stop lamp due to a melted socket is encountered in a Firenza Style 37 or Cutlass Ciera Style 37, both sockets must be installed using part number 5972532 available from GMSPO. All service stock of this part uses a new heat resistant material. The production stock was corrected beginning with the following VIN breakpoints:

JG307649 J9367993 J2336554

#### WARRANTY INFORMATION:

Labor Operation Number: N1000 Labor Time: 0.2 hrs. Part Number 5972532 (2 pieces)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.