For 1990-2009 cars

# SQUAWK NOISE FROM THE REAR NEW SPRING UPPER INSULATOR

#### MODELS/YEARS 1982-88 FIRENZA MODELS 1985-90 CUTLASS CALAIS MODELS

Customers may comment about a squawk or squeak coming from the rear of the vehicle, particularly during cold weather (temperature 40 degrees F or colder). This condition may be caused by distortion of the rear spring upper insulator, resulting in a squeak or squawk noise. This condition may be corrected by installing new rear spring upper insulators, P/N 22555689, following the service manual procedure.

#### IMPORTANT: New P/N 22555689 will temporarily be supplied with P/N 1001 7875 molded into the side. New part is identified by a white stripe on the edge of the insulator.

Parts are currently available from GMSPO.

#### WARRANTY INFORMATION:

Labor Operation Number: E5057 Labor Time: 0.6 Hour Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.