For 1990-2009 cars

### Removal Procedure

1. Remove the surge tank. Refer to Radiator Surge Tank Replacement .
2. Disconnect the electrical connector from the sensor.
3. Remove the surge tank.
4. Remove the sensor.

### Installation Procedure

1. Install the sensor.
2. Install the surge tank.
3. Connect the electrical connector to the sensor.
4. Install the surge tank. Refer to Radiator Surge Tank Replacement .