For 1990-2009 cars

# TEA KETTLE TYPE WHISTLE OR HIGH PITCH WHINE FROM ENGINE

TEA KETTLE TYPE WHISTLE OR HIGH PITCH WHINE NOISE FROM ENGINE (REPLACE ENGINE OIL PUMP)

SOME 1989 CUTLASS CALAIS MODELS BUILT IN SEPTEMBER,1988, EQUIPPED WITH A QUAD 4 (LD2) ENGINE

#### CONDITION:

---------- Some September built 1989 Cutlass Calais models with a 2.3L Quad 4 engine, prior to engine unit number D181098, may exhibit a tea kettle type whistle or high pitch whine noise with a warm engine in the 900 to 1400 RPM range.

#### NOTE: The month and year of vehicle manufacture is printed on the vehicle certification label. This labor is located on the rear face of the driver's door.

Refer to the following illustration for engine unit number label location.

#### CAUSE:

------ This noise is a result of a high frequency resonance created within the oil pump assembly. This condition does not affect the durability or performance of the oil pump.

#### CORRECTION:

----------- This condition can be corrected by replacing the engine oil pump, part number 22538689. Parts are expected to be available on November 14,1988. Until then normal part orders will not be accepted by GMSPO. Only verifiable emergency VIP orders will be accepted. GMSPO will make every effort to obtain parts. All parts will be placed on 400 control to waive VIP surcharges. However, the part will be shipped premium transportation at dealer's expense. All other order types will be canceled as incorrectly ordered while the 400 control is in place.

Refer to Page 6A7-35 of the 1989 Cutlass Calais New Product Service Manual for engine oil pump removal and installation procedure.

#### WARRANTY INFORMATION:

Labor Operation Number: J1020 Labor Time: .9 hour

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.