For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel insert, front door only. Refer to Front Side Door Trim Panel Insert Replacement .
2. Remove the door handle bezel. Refer to Door Handle Bezel Replacement .
3. Remove the window regulator handle, if equipped. Refer to Door Window Regulator Handle Replacement .
4. Remove the power window switch, if equipped. Refer to Front Side Door Window Switch Replacement or Power Accessory Switch Panel Replacement .
5. Remove the door handle plug (3), pry off with a flat bladed tool.
6. Remove the door trim handle screws (2).
7. Remove the door trim panel (1) from the retainers (4). Start at the bottom rear corner and gently pry outward.
8. Remove the door trim panel (1) from the vehicle.

### Installation Procedure

1. Install the door trim panel (1) to the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the door trim handle screws (2).

Tighten
Tighten the screws to 10 N·m (89 lb in).

3. Install the door handle plug (3). Ensure that the unit is retained.
4. Install the power window regulator handle, if equipped. Refer to Door Window Regulator Handle Replacement .
5. Install the power window switch, if equipped. Refer to Front Side Door Window Switch Replacement or Power Accessory Switch Panel Replacement
6. Install the door handle bezel. Refer to Door Handle Bezel Replacement .
7. Install the front door trim panel insert. Refer to Front Side Door Trim Panel Insert Replacement .