For 1990-2009 cars

Table 1: | Inflator Module, Driver
Table 2: | Inflator Module, Passenger
Table 3: | Sensing Diagnostic Module (SDM)

#### Inflator Module, Driver

Connector Part Information |

• | 12124635

• | 2-Way M Metri-Pack 280 Series (YEL)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 347 | SIR Inflator Feed-Driver
B | DK GRN | 348 | SIR Inflator Output-Driver

#### Inflator Module, Passenger

Connector Part Information |

• | 12110288

• | 2-Way F Metri-Pack 280 Series (YEL)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT/BLK | 1403 | SIR Inflator Feed-Passenger
B | DK GRN/WHT | 1404 | SIR Inflator Output-Passenger

#### Sensing Diagnostic Module (SDM)

Connector Part Information |

• | 15326335

• | 12-Way F Metri-Pack 280 Series (YEL)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WHT/BLK | 1403 | SIR Inflator Feed-Passenger
2 | WHT | 347 | SIR Inflator Feed-Driver
3 | DK GRN | 348 | SIR Inflator Output-Driver
4 | DK GRN/WHT | 1404 | SIR Inflator Output-Passenger
5 | TAN | 800 | Serial Data Signal-UART (8192 BAUD-Primary)
6 | BLK/WHT | 1751 | SIR Ground
7 | BRN | 358 | SIR Indicator Lamp Output
8 | BLK/WHT | 238 | Seat Belt Switch Signal
9 | -- | -- | Not Used
10 | YEL | 1139 | Fuse Output-Ignition 1 (Type III Fuse-SIR)
11-12 | -- | -- | Not Used