For 1990-2009 cars

In order to overhaul, follow the sequence below.

1. Torque Converter Removal
2. Transmission Holding Fixture Assemble
3. Stub Shaft Removal
4. Output Shaft Speed Sensor Removal
5. Oil Pan and Gasket Removal
6. Oil Filter/Seal, Oil Level Control Valve Removal
7. Oil Feed Pipes Removal
8. Intermediate/4th Servo Removal
9. Low and Reverse Servo Removal
10. Case Side Cover Removal
11. Oil Pump and Oil Pump Shaft Removal
12. Wire Harness Disconnect
13. Transmission Fluid Pressure (TFP) Switch Removal
14. Control Valve Body Assembly and Gasket Removal
15. Spacer Plate and Gasket Removal
16. Checkball Removal
17. Manual Valve Clip Removal
18. Channel Plate and Gasket Removal
19. Accumulator Spring Removal
20. Output Shaft Sleeve Removal
21. Drive, Driven Sprockets, Drive Link Removal
22. Input Speed Sensor Removal
23. Wiring Harness Removal
24. Driven Sprocket Support Assembly Removal
25. 2nd Clutch Plates Removal
26. Reverse Input Clutch Housing Removal
27. Intermediate 4th Band Removal
28. Direct/Coast Clutch and Reaction Gear Set Removal
29. Input Carrier and Reaction Gear Assembly Removal
30. Input Internal Gear, Forward Clutch Hub Removal
31. Forward Clutch and Low/Reverse Band Removal
32. Forward Clutch Support, Low Roller Clutch Removal
33. Output Shaft and Final Drive Assembly Removal
34. Final Drive Internal Gear Removal
35. Manual Shaft, Detent Lever, Park Lock Removal
36. Transmission Cooler Line Seals Removal
37. Torque Converter Seal Removal
38. Drive Sprocket Support Removal
39. Right Hand Axle Seal Removal
40. Case Inspection
41. Actuator Guide Replacement
42. Drive Sprocket Support Installation
43. Torque Converter Seal Installation
44. Transmission Cooler Line Seals Installation
45. Manual Shaft, Detent Lever, Park Lock Installation
46. Final Drive Assembly Disassemble
47. Final Drive Assembly Assemble
48. Final Drive Pinion End Play Check
49. Fretting Ring, Final Drive Internal Gear Install
50. Forward Clutch Support, Roller Clutch Disassemble
51. Forward Clutch Support, Low Roller Clutch Assemble
52. Forward Clutch Support, Low Roller Clutch Install
53. Forward Clutch Disassemble
54. Forward Clutch Assemble
55. Forward Clutch Functional Air Check
56. Low/Reverse Band Installation
57. Forward Clutch Assembly Installation
58. Input Internal Gear, Forward Clutch Hub Disassemble
59. Input Internal Gear, Forward Clutch Hub Assemble
60. Input Internal Gear, Forward Clutch Hub Install
61. Reaction Internal Gear, Input Carrier Disassemble
62. Input Carrier Pinion Gear Clearance Check
63. Reaction Internal Gear, Input Carrier Assemble
64. Reaction Internal Gear, Input Carrier Installation
65. Direct/Coast Clutch, Reaction Carrier Disassemble
66. Reaction Carrier Pinion Clearance Check
67. Direct/Coast Clutch, Reaction Carrier Assemble
68. Direct and Coast Clutch Functional Air Checks
69. Direct/Coast Clutch, Reaction Carrier Installation
70. Selective Washer Measurement and Installation
71. Reverse Input and 2nd Roller Clutch Disassemble
72. Reverse Input and 2nd Roller Clutch Assemble
73. Reverse Clutch Functional Air Check
74. Reverse Input and Second Roller Clutch Installation
75. Intermediate Fourth Band Assembly Installation
76. Second Clutch Plate Installation
77. Driven Sprocket Support Assembly Disassemble
78. Drive Sprocket Support Assemble
79. 2nd Clutch Functional Air Check
80. Wiring Harness Connection
81. Input Speed Sensor Installation
82. Drive, Driven Sprockets and Drive Link Disassemble
83. Drive, Driven Sprockets and Drive Link Assemble
84. Drive Sprocket, Driven Sprocket, and Drive Link Installation
85. Channel Plate Assembly Disassemble
86. Channel Plate Assembly Assemble
87. Accumulator Springs Installation
88. Channel Plate Assembly Installation
89. Manual Valve Link Installation
90. Spacer Plate and Gaskets Installation
91. Control Valve Body Disassemble
92. Control Valve Body Assemble
93. Control Valve Assembly and Transmission Fluid Pressure (TFP) Switch Installation
94. Oil Pump Clean and Inspect
95. Oil Pump Assembly Installation
96. Side Cover/Gaskets, Disassemble, Assemble, Install
97. Output Shaft Sleeve Assemble
98. Output Shaft and Sleeve Assembly Installation
99. Side Cover Axle Seal Installation
100. Stub Shaft Sleeve Assembly Installation
101. Right Hand Axle Seal Assemble
102. Vehicle Speed Sensor Installation
103. Intermediate/4th Servo Disassemble
104. Intermediate/4th Servo Assemble and Installation
105. Low and Reverse Servo Disassemble
106. Low and Reverse Servo Assemble and Installation
107. Oil Feed Pipes Assemble
108. Filter Assembly and Seal Installation
109. Oil Level Control Valve Installation
110. Oil Pan and Gasket Installation
111. Torque Converter Installation