For 1990-2009 cars

# POWER STRG. RACK & PINION SHORT GEAR SERV. P/N'S

#### MODELS/YEARS: 1982-86 FIRENZA MODELS AND 1985-86 CALAIS MODELS

1987 style center take-off power rack and pinion "short gears" will now be provided as a service replacement for most applications on 1982-86 Firenza and 1985-86 Calais models.

To install the 1987 style gear on prior year models, the short gear package will include one (1) 26000412 coupling assembly, one (1) 26001492 RH mounting grommet, and one (1) 22823112 line retainer. An instruction sheet will be included.

#### REPLACEMENT APPLICATION

New Short Gear Year Model Part Number ---- ----- --------------

1982-84 Firenza 26008036

1985-86 Firenza (except F41 suspension) with 1.8L or 26008040 2.0L engine

1985-86 Firenza with 1.8L or 2.0L engine and F41 26008038 suspension

1985-86 Firenza with LB6 2.8L engine 7849109*

1985-86 Calais (except F41 suspension) 26008040

1985-86 Calais with F41 suspension 26008038

1985-86 Calais with N78 wheels and F41 suspension 26008039

*This application remains unchanged

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.