For 1990-2009 cars

## Backup Lamp Replacement Oldsmobile

### Removal Procedure

1. Remove the taillamp. Refer to Tail Lamp Replacement .
2. Disconnect the electrical connector (7).
3. Remove the bulb (3) from the socket.

### Installation Procedure

1. Install the bulb (3) to the socket.
2. Connect the electrical connector (7).
3. Install the taillamp. Refer to Tail Lamp Replacement .

## Backup Lamp Replacement Chevrolet

### Removal Procedure

1. Remove the taillamp. Refer to Tail Lamp Replacement .
2. Disconnect the electrical connector (6).
3. Remove the bulb (5) from the socket.

### Installation Procedure

1. Install the bulb (5) to the socket.
2. Connect the electrical connector (6).
3. Install the taillamps. Refer to Tail Lamp Replacement .