For 1990-2009 cars

Table 1: | Washer Motor
Table 2: | Washer Solvent Level Sensor
Table 3: | Wiper Motor Assembly
Table 4: | Wiper Switch Assembly

#### Washer Motor

Connector Part Information |

• | 12052641

• | 2-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 228 | Windshield Washer Pump Motor Feed
B | BLK | 1350 | Ground

#### Washer Solvent Level Sensor

Connector Part Information |

• | 12162195

• | 2-Way F Metri-Pack 150.2 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/WHT | 99 | Windshield Washer Fluid Level Sensor Signal
B | BLK | 1350 | Ground

#### Wiper Motor Assembly

Connector Part Information |

• | 12129125

• | 5-Way F Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 150 | Ground
B | YEL | 143 | Fuse Output, ACCY (Type III Fuse)
C | PPL | 92 | Windshield Wiper Motor Feed (HIGH)
D | DK GRN | 113 | Windshield Wiper Switch Signal (ON)
E | GRY | 112 | Windshield Wiper Switch Signal (LOW/PULSE)

#### Wiper Switch Assembly

Connector Part Information |

• | 12041429

• | 5-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 92 | Windshield Wiper Motor Feed (HIGH)
B | RED | 228 | Windshield Washer Pump Motor Feed
C | YEL | 143 | Fuse Output, ACCY (Type III Fuse)
D | GRY | 112 | Windshield Wiper Switch Signal (LOW/PULSE)
E | DK GRN | 113 | Windshield Wiper Switch Signal (ON)