For 1990-2009 cars

# INSTRUMENT PANEL SQUEAK (INSTALL CLIPS)

#### VEHICLES AFFECTED: 1987-89 OLDSMOBILE CUTLASS CIERA

#### Condition:

--------- A squeak or itch (plastiC tO plastic Sound) may be heard in the instrument panel (IP) area of the 1987 to 1989 Oldsmobile Cutlass Ciera.

#### Cause:

----- The instrument cluster lens is not properly retained to the cluster body, and may cause an itch or squeak. This condition was corrected with the following VIN breakpoints:

Framingham KG306321 Ste. Therese K2323674

#### Correction:

----------- 1. Disconnect negative battery cable.

2. Remove the instrument cluster following Service Manual instructions.

3. Install two clips, P/N 16130132, at the lower corners of the cluster, as shown in the illustration (right hand side shown). The clip should be rolled onto the glass, with the toothed side put on first.

4. Reinstall instrument cluster, reconnect negative battery cable, and check cluster for proper operation.

Warranty Information: Use most applicable Labour Operation and time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.