For 1990-2009 cars

# CHOKE HEATER RELAY LOCATION 1981 CUTLASS

THE CHOKE HEATER RELAY ON 1981 CUTLASS MODELS EQUIPPED WITH THE 3.8L V6 AND U-14 RALLYE INSTRUMENT CLUSTER HAS BEEN RELOCATED FROM THE LEFT FRONT FENDER TO THE RIGHT SIDE OF THE BRAKE BOOSTER.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.