For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Drivers Side Six-Way Power Seat Switch Screw | 1 N·m | 9 lb in
Front Seat Manual Adjuster Bolts | 40 N·m | 30 lb ft
Recliner Cable Retaining Screw | 4 N·m | 35 lb in
Seat Adjuster To Seat Cushion Frame Bolt | 25 N·m | 18 lb ft
Seat Cushion Outer Trim Panel Screw | 1 N·m | 9 lb in
Seat Recliner Handle Screw | 1 N·m | 9 lb in
Seat Recliner To Seat Back Bolt | 3 N·m | 27 lb in
Seat Recliner To Seat Cushion Frame Bolt | 25 N·m | 18 lb ft
Split/Folding Rear Seat Back Bolster Bolt | 12 N·m | 106 lb in
Split/Folding Rear Seat Back Folding Armrest Nut | 10 N·m | 89 lb in
Split/Folding Rear Seat Back Folding Armrest Screw | 10 N·m | 89 lb in
Split/Folding Rear Seat Back Strike Bolt | 25 N·m | 18 lb ft
Stationary Rear Seat Back Bolt | 12 N·m | 106 lb in
Vertical Actuator Jackscrew Nuts | Fully Driven, Seated, Not Stripped
Vertical Actuator Screws | 16 N·m | 12 lb ft