For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Turn the engine OFF.
2. Turn the ignition switch to the RUN position.
3. Attempt to shift the vehicle out of PARK.

The vehicle does not shift out of PARK.

• | The vehicle shifts out of PARK without the brake pedal depressed.

• | Automatic Transmission Shift Lock Control Inoperative

2 |

1. Depress the brake pedal.
2. Attempt to shift the vehicle out of PARK.

The vehicle shifts out of PARK.

• | The vehicle does not shift out of PARK with the brake pedal depressed.

• | Automatic Transmission Shift Lock Control Always On With Ignition in RUN

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.