For 1990-2009 cars

Table 1: | Cruise Control Brake Switch
Table 2: | Cruise Control Module
Table 3: | Cruise Control Switch C1
Table 4: | Cruise Control Switch C2

#### Cruise Control Brake Switch

Connector Part Information |

• | 12041433

• | 2-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 341 | Fuse Output, Ignition 3
B | PPL | 420 | Brake Pedal Switch Output (Torque Converter Clutch)

#### Cruise Control Module

Connector Part Information |

• | 12177081

• | 10-Way F Global Terminal 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 397 | Cruise Control Switch Output (ON)
B | DK BLU | 84 | Cruise Control Switch Signal (SET/COAST)
C | GRY/BLK | 87 | Cruise Control Switch Signal (RESUME/ACCEL)
D | PPL | 420 | Brake Pedal Switch Output (TCC)
E | BLK | 1350 | Ground
F | BRN | 341 | Fuse Output, Ignition 3
G | LT BLU | 20 | Stoplamp Feed
H | DK GRN | 83 | Cruise Control Signal (Disengage)
J | LT BLU/BLK | 396 | Cruise Control Signal (Engaged)
K | DK GRN/WHT | 817 | Vehicle Speed Signal (4000 Pulses per Mile)

#### Cruise Control Switch C1

Connector Part Information |

• | 12092162

• | 4-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 441 | Fuse Output, Ignition 3
B | DK BLU | 84 | Cruise Control Switch Signal (SET/COAST)
C | GRY/BLK | 87 | Cruise Control Switch Signal (RESUME/ACCEL)
D | GRY | 397 | Cruise Control Switch Output (ON)

#### Cruise Control Switch C2

Connector Part Information |

• | 12064760

• | 4-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 441 | Fuse Output, Ignition 3
B | DK BLU | 84 | Cruise Control Switch Signal (SET/COAST)
C | GRY/BLK | 87 | Cruise Control Switch Signal (RESUME/ACCEL)
D | GRY | 397 | Cruise Control Switch Output (ON)