For 1990-2009 cars

# TAIL LAMP 'ROCKET' EMBLEM FALLS OFF (NEW ROCKET EMBLEM)

1987-88 CUTLASS CALAIS COUPE AND SEDAN

When it is necessary to replace the rocket emblem on the tail lamp assembly due to loss or damage, do not replace the complete lamp assembly. The rocket emblem, without the chrome bezel, is now available through GMSPO under part number 16507586.

A new "S" shaped adhesive pattern was used in production after November 12, 1987 and cars built after VIN JM233546 will have the new emblem adhesive pattern.

Install new emblem as follows:

1. Remove old adhesive and clean dirt, wax or oil from the bezel.

2. Refer to Figure 1 and apply RTV adhesive as shown to the back of the emblem and install into bezel. Follow the adhesive manufacturers instructions for retention and cure times.

#### WARRANTY INFORMATION:

Labor Operation Number: B8700 Labor Time: 0.2hrs. Part Number: 16507586

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.