For 1990-2009 cars

Table 1: | Camshaft Position (CMP) Sensor
Table 2: | Crankshaft Position (CKP) Sensor
Table 3: | Engine Coolant Temperature (ECT) Sensor
Table 4: | Engine Oil Pressure Sensor
Table 5: | Evaporative Emission (EVAP) Canister Purge Valve
Table 6: | Evaporative Emission (EVAP) Canister Vent Solenoid
Table 7: | Ignition Control Module
Table 8: | Fuel Injectors
Table 9: | Fuel Tank Pressure Sensor
Table 10: | Fuel Tank Module
Table 11: | Pre Converter Oxygen Sensor (O2S1)
Table 12: | Post Converter Heated Oxygen Sensor (HO2S 2)
Table 13: | Idle Air Control (IAC) Valve
Table 14: | Intake Air Temperature (IAT) Sensor
Table 15: | Knock Sensor
Table 16: | Manifold Absolute Pressure (MAP) Sensor
Table 17: | Throttle Position (TP) Sensor
Table 18: | Park/Neutral Position Switch C1
Table 19: | Park/Neutral Position Switch C2
Table 20: | Vehicle Speed Sensor (VSS)

#### Camshaft Position (CMP) Sensor

Connector Part Information |

• | 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN/WHT | 633 | Camshaft Position (CMP) Sensor Signal
B | PNK/BLK | 632 | Camshaft Position Sensor Return
C | RED | 631 | Camshaft Sensor Feed (12 Volt Reference)

#### Crankshaft Position (CKP) Sensor

Connector Part Information |

• | 12162194

• | 2-Way F Metri-Pack 150.2 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 574 | Crankshaft Position Sensor Return
B | YEL | 573 | Crankshaft Position Sensor Signal

#### Engine Coolant Temperature (ECT) Sensor

Connector Part Information |

• | 12162195

• | 2-Way F Metri-Pack 150.2 Series Pull to Seat Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/WHT | 2761 | Sensor Return
B | YEL | 410 | Coolant Temperature Sensor Signal

#### Engine Oil Pressure Sensor

Connector Part Information |

• | 12065299

• | 1-Way F Metri-Pack 150 Series Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/BLK | 231 | Oil Pressure Switch Signal

#### Evaporative Emission (EVAP) Canister Purge Valve

Connector Part Information |

• | 12052643

• | 2-Way F Metri-Pack 150 Series (RED)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 241 | Fuse Output-Ignition 3
B | DK GRN/WHT | 428 | Canister Purge Solenoid Output

#### Evaporative Emission (EVAP) Canister Vent Solenoid

Connector Part Information |

• | 12059863

• | 2-Way F Metri-Pack 150 Series Sealed (BRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 241 | Fuse Output-Ignition 3
B | WHT | 1310 | Canister Vent Valve Solenoid Output

#### Ignition Control Module

Connector Part Information |

• | 12162838

• | 11-Way F Metri-pack 150.2 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 423 | Electronic Spark Timing Control Signal
B | ORN | 406 | Electronic Spark Timing Control Signal B
C-E | -- | -- | Not Used
F | YEL | 573 | Crankshaft Position Sensor Signal
G | PPL/WHT | 430 | Electronic Spark Timing High Reference Signal
H | RED/BLK | 453 | Electronic Spark Timing Low Reference Signal
J | PPL | 574 | Crankshaft Position Sensor Return
K | BLK | 450 | Ground
L | PNK | 239 | Fuse Output, Ignition 1

#### Fuel Injectors

Connector Part Information |

• | 15326179

• | 2-Way F Micro-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1A | GRY | 120 | Fuel Pump Motor Feed
1B | BLK | 1744 | Fuel Injector #1Output
2A | GRY | 120 | Fuel Pump Motor Feed
2B | LT GRN/BLK | 1745 | Fuel Injector #2 Output
3A | GRY | 120 | Fuel Pump Motor Feed
3B | PNK/BLK | 1746 | Fuel Injector #3Output
4A | GRY | 120 | Fuel Pump Motor Feed
4B | LT BLU/BLK | 844 | Fuel Injector #4Output

#### Fuel Tank Pressure Sensor

Connector Part Information |

• | 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 2759 | MAP Sensor Return
B | DK GRN | 890 | Fuel Tank Pressure Sensor Signal
C | GRY | 2709 | 5V Sensor Reference

#### Fuel Tank Module

Connector Part Information |

• | 12160482

• | 4-Way F Metri-Pack 150 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 1589 | Fuel Gauge Sensor Signal
B | GRY | 120 | Fuel Pump Motor Feed
C | BLK | 150 | Ground
D | BLK/WHT | 2759 | Fuel Gauge Sensor Ground

#### Pre Converter Oxygen Sensor (O2S1)

Connector Part Information |

• | 12065172

• | 1-Way F Metri-Pack 280 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 412 | Oxygen Sensor Signal

#### Post Converter Heated Oxygen Sensor (HO2S 2)

Connector Part Information |

• | 12160825

• | 4-Way M Metri-pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/WHT | 1669 | Oxygen Sensor Return-Left (Rear of Catalytic Converter)
B | PPL/WHT | 1668 | Oxygen Sensor Signal-Left (Rear of Catalytic Converter)
C | BLK | 250 | Ground
D | BRN | 241 | Fuse Output, Ignition 3

#### Idle Air Control (IAC) Valve

Connector Part Information |

• | 12162190

• | 4-Way F Metri-Pack 150.2 Series Pull to Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN/BLK | 444 | Idle Air Control (IAC) Valve Motor Feed-Coil B Low
B | LT GRN/WHT | 1749 | Idle Air Control (IAC) Valve Motor Feed-Coil B High
C | LT BLU/BLK | 1748 | Idle Air Control (IAC) Valve Motor Feed-Coil A Low
D | LT BLU/WHT | 1747 | Idle Air Control (IAC) Valve Motor Feed-Coil A High

#### Intake Air Temperature (IAT) Sensor

Connector Part Information |

• | 12162199

• | 2-Way F Metri-Pack 150.2 Series Pull to Seat (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 2760 | Sensor Return
B | TAN | 472 | Intake Air Temperature Signal

#### Knock Sensor

Connector Part Information |

• | 12077900

• | 2-Way F Metri-Pack 280 Series Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 496 | Knock Sensor Signal #1
B | GRY | 1716 | Knock Sensor Signal Return

#### Manifold Absolute Pressure (MAP) Sensor

Connector Part Information |

• | 12129946

• | 3-Way F Metri-Pack 150 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN/BLK | 469 | Manifold Absolute Pressure (MAP) Sensor Return
B | LT GRN | 432 | Manifold Absolute Pressure (MAP) Sensor Signal
C | BRN | 2704 | Manifold Absolute Pressure (MAP) Sensor 5V Reference

#### Throttle Position (TP) Sensor

Connector Part Information |

• | 12110192

• | 3-Way F Metri-Pack 150 Series Pull To Seat (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY/BLK | 2701 | Throttle Position (TP) Sensor 5V Reference
B | BLK | 2752 | Throttle Position Sensor Return
C | DK BLU | 417 | Throttle Position Sensor Signal

#### Park/Neutral Position Switch C1

Connector Part Information |

• | 12129840

• | 7-Way F Metri-Pack Mixed Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 1737 | Transaxle Mounted Neutral Safety Switch Output-Park/Neutral
B | PNK | 539 | Fuse Output, Ignition 1
C | LT GRN | 275 | Transaxle Mounted Neutral Safety Switch Output-Park
D | BLKWHT | 451 | Engine Control Module Ground
E | PPL | 6 | Starter Solenoid Feed
F | LT GRN | 24 | Backup Lamp Feed
G | YEL | 5 | Ignition Switch Output-Crank

#### Park/Neutral Position Switch C2

Connector Part Information |

• | 12191757

• | 4-Way F Metri-Pack 150 Series Sealed (Natural)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT | 776 | Transmission Position Switch Signal-Parity Bit
B | YEL | 772 | Transmission Position Switch Signal-Bit 2
C | GRY | 773 | Transmission Position Switch Signal-Bit 3
D | BLK/WHT | 771 | Transmission Position Switch Signal-Bit 1

#### Vehicle Speed Sensor (VSS)

Connector Part Information |

• | 12162195

• | 2-Way F Metri-Pack 150.2 Series Pull to Seat Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 401 | Vehicle Speed Sensor (VSS) Return
B | YEL | 400 | Vehicle Speed Sensor (VSS) Signal