For 1990-2009 cars

# MULTIPLE DRIVEABILITY CONCERNS FOR 2.5L ENGINE

#### MODELS/YEARS 1987-89 CUTLASS CALAIS AND CUTLASS CIERA

This bulletin cancels and supersedes Dealer Technical Bulletin 88-T-54.

This bulletin contains new and revised calibrations to address additional driveability conditions.

Some 1987-89 Cutlass Calais and Cutlass Ciera models may exhibit one or more of the following driveability conditions:

1. Hard Hot Engine Restart 2. Intermittent Higher Than "Normal" Idle 3. Spark Knock (Detonation) 4. Code 42

If these conditions cannot be addressed through normal service procedures, they may be repaired by installing the appropriate hardware as outlined below.

#### SERVICE PROCEDURE:

1. Use a scanner to determine the PROM I.D. that is currently in the vehicle.

2. Look for that PROM I.D. in Table 1 or Table 2 as indicated below, and select the corresponding required parts:

3. If the major condition is Hard Hot Engine Restart, use Table 1.

#### WARRANTY INFORMATION:

To repair Hard Hot Engine Restart with or without any of the above driveability conditions:

Labor Operation Number: T1314 Labor Time for the following car lines: Cutlass Ciera Cutlass Calais 1.6 Hr. 1.7 Hr. Trouble Code: 92

4. If the major condition is Intermittent High Idle (similar to cold fast idle) manual transaxle, Spark Knock, and/or Code 42, use Table 2.

#### WARRANTY INFORMATION:

To repair Intermittent Higher Than "Normal" Idle, Spark Knock, and/or Code 42:

Labor Operation Number: J6364

5. Install the new parts and verify that the driveability conditions have been corrected. Table 1 -------

VEHICLE CONFIGURATION REQUIRED PARTS(*) --------------------- ----------------- CURRENT NEW PROM NEW NEW PROM FUEL FUEL CAR INST. I.D. PROM PROM I.D. SENDER PUMP LINE MY TRANS CLUSTER (SCAN) P/N LABEL (SCAN) P/N P/N ---- -- ----- ------- ------ --- ----- ------ --- ---- A 87-88 AUTO D or A 2702 16143580 ATBY 3551 25093744 25115764 A 87-88 AUTO D or A 2782 16143580 ATBY 3551 25093744 25115764 A 87-88 AUTO D or A 9522 16143580 ATBY 3551 25093744 25115764

N 87 AUTO A 1272 16143457 ATBU 3521 25092778 25115925 N 87 AUTO D 1272 16143457 ATBU 3521 25092769 25115925 N 87 AUTO D 9532 16143457 ATBU 3521 25092769 25115925 N 87 AUTO A 9532 16143457 ATBU 3521 25092778 25115925 N 87 MAN D 1282 16143452 ATBR 3491 25092769 25115925 N 87 MAN A 1282 16143452 ATBR 3491 25092778 25115925 N 87 MAN D 9542 16143452 ATBR 3491 25092769 25115925 N 87 MAN A 9542 16143452 ATBR 3491 25092778 25115925

CARLINE

A = Cutlass Ciera N = Cutlass Calais

#### NOTE: In addition to the required parts above, each application in this table also requires the installation of a "rubber bumper" package (P/N 25004553) and a "pulsator" package (P/N 25094266).

#### NOTE: D = Digital A = Analog

#### Table 2

VEHICLE CONFIGURATION REQUIRED PARTS --------------------- --------------- CURRENT NEW NEW CAR MODEL PROM I.D. NEW PROM PROM PROM I.D. PROM I.D. LINE YEAR TRANS (scanner) PKG.P/N LABEL (scanner) ---- ----- ----- --------- -------- ----- --------- A 87-88 AUTO 1222 16143580 ATBY 3551 A 87-88 AUTO 2702 16143462 ATCC 3591 A 87-88 AUTO 2782 16143462 ATCC 3591 A 87-88 AUTO 5402 16143580 ATBY 3551 A 87-88 AUTO 9522 16143462 ATCC 3591 A 88-89 AUTO 1532 16143545 ATBM 3461 A 88-89 AUTO 5132 16143545 ATBM 3461 A 88-89 AUTO 5932 16143545 ATBM 3461 A(*) 89 AUTO 0671 16143467 ATCD 3601

N 87 AUTO 1272 16143466 ATBP 3481 N 87 AUTO 9532 16143466 ATBP 3481 N 87 MAN 1282 16143463 ATBL 3451 N 87 MAN 9542 16143463 ATBL 3451 N 87-88 AUTO 1232 16143457 ATBU 3521 N 87-88 AUTO 6402 16143457 ATBU 3521 N 87-88 MAN 1242 16143452 ATBR 3491 N 87-88 MAN 6412 16143452 ATBR 3491

(*) NOTE: Only applicable to vehicles equipped with 215/60-R14 tires (RPO QMB).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.