For 1990-2009 cars

#### Instrument Cluster

Connector Part Information |

• | 12110088

• | 24-Way F Micro-Pack 100 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | ORN | 1440 | Fuse Output, Battery (Type III Fuse)
A2 | LT BLU/BLK | 1322 | Serial Data SPI Data Transmit
A3 | -- | -- | Not Used
A4 | BLK/WHT | 151 | Power Mirror Motor Ground (Clean)
A5 | GRY | 8 | IP Lamp Feed
A6 | -- | -- | Not Used
A7 | WHT | 121 | Tachometer Signal
A8 | DK GRN/WHT | 817 | Vehicle Speed Signal (4000 Pulses per Mile)
A9 | YEL | 1321 | Serial Data SPI Data Receive
A10 | PNK/BLK | 1323 | Serial Data SPI Clock
A11 - A12 | -- | -- | Not Used
B1 | DK BLU | 15 | Turn Signal Lamp Feed, Left Front
B2 | LT BLU | 14 | Turn Signal Lamp Feed, Left Front
B3-B8 | -- | -- | Not Used
B9 | PPL | 1600 | Fuse Output, Ignition 0 (Type III Fuse)
B10 | BLK/WHT | 151 | Ground
B11 | BRN/WHT | 419 | Check Engine Indicator Lamp Output
B12 | BRN | 358 | SIR Indicator Lamp Output