For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Door Check Link to Hinge Pillar Bolt | 9 N·m | 80 lb in
Door Handle Bezel Screw | 2 N·m | 20 lb in
Door Hinge Bolts | 25 N·m | 18 lb ft
Door Hinge Nuts | 25 N·m | 18 lb ft
Door Hold Open Bolts | 25 N·m | 18 lb ft
Door Locating Pin Bolt | 10 N·m | 89 lb in
Door Lock Actuator Screws | 6 N·m | 53 lb in
Door Lock Striker Bolts | 25 N·m | 18 lb ft
Door Locking System Module Bolt | 10 N·m | 89 lb in
Door Locking System Module Nuts | 10 N·m | 89 lb in
Door Lower Energy Absorber Screws | 10 N·m | 89 lb in
Door Trim Handle Screws | 10 N·m | 89 lb in
Front Window Run Channel Bolt | 10 N·m | 89 lb in
Front Window Run Channel Screw | 2 N·m | 18 lb in
Outside Rearview Mirror Nuts | 10 N·m | 89 lb in
Rear Door Lock Screws | 6 N·m | 53 lb in
Rear Door Window to Inner Panel Bolt | 10 N·m | 89 lb in
Rear Door Window to Inner Panel Screw | 2 N·m | 18 lb in
Rear Inside Handle Screws | 1 N·m | 9 lb in