For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Set the entire seat adjuster switch to ANY position. | The seat will move in the direction that the seat adjuster switch is set. | Power Seat Inoperative
2 | Set the entire seat adjuster switch to the FORWARD and then the BACK position. | The seat will move forward and backward. | Power Seat Does Not Move Forward/Rearward
3 | Set the front height switch to the UP and then the DOWN position. | The front of the seat will tilt up and down. | Power Seat Does Not Tilt Forward
4 | Set the rear height switch to the UP and then the DOWN position. | The rear of the seat will tilt up and down. | Power Seat Does Not Tilt Rearward
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.