For 1990-2009 cars

### Removal Procedure

1. Remove the left and right rear taillamp assemblies. Refer to Tail Lamp Replacement in Lighting Systems.
2. Remove the fascia retaining nuts from the inside rear compartment.
3. Remove the bolts (1) from the rear fascia (3) in the rear wheel housing.
4. Remove the push-in retainers (2) from the top edge of the fascia (3).
5. Remove the push-in retainers (2) from the lower edge of the fascia (3).
6. Remove the rear fascia (3) from the impact bar (1).
7. Twist the license lamp socket from the fascia (3).
8. Remove the side reinforcement screws (2) from each side of the fascia (4).
9. Remove the side reinforcements (1) from the fascia (4).

### Installation Procedure

1. Install the side reinforcements (1) to the fascia (4).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the side reinforcement screws (2) to the fascia (4).

Tighten
Tighten the screws to 6 N·m (53 lb in).

3. Install the rear fascia (3) to the impact bar (1).
4. Install the license lamp socket to the fascia (3).
5. Install the fascia retaining nuts from the inside rear compartment.

Tighten
Tighten the nuts to 10 N·m (89 lb in).

6. Install the bolts (1) to the rear fascia on the rear wheel housing.

Tighten
Tighten the bolts to 6 N·m (53 lb in).

7. Install the push-in retainers (2) to the lower edge of the fascia (3).
8. Install the push-in retainers (2) to the top edge of the fascia (3).
9. Install the left and right rear taillamp assemblies. Refer to Tail Lamp Replacement in Lighting Systems.