For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Fuel Tank Filler Door Screws | 1 N·m | 9 lb in
Hinge Assembly to Body Bolts | 11 N·m | 97 lb in
Rear Compartment Lid Applique Nuts | 1 N·m | 9 lb in
Rear Compartment Lid Lock Bolts | 11 N·m | 97 lb in
Rear Compartment Lid Lock Striker Nuts | 7 N·m | 62 lb in
Rear Compartment Lid to Hinge Bolts | 10 N·m | 89 lb in
Taillamp Nuts | 2 N·m | 18 lb in