For 1990-2009 cars

Application | Fluid/Lubricant
--- | ---
Automatic Transaxle | DEXRON®-III Automatic Transmission Fluid (or equivalent)
Engine Coolant | A 50/50 mixture of clean water (preferably distilled) and use only GM Goodwrench® DEX-COOL® or Havoline® DEX-COOL® (orange-colored, silicate-free) coolant, conforming to GM Specification 6277M
Chassis Lubrication | Chassis Lubricant aerosol (GM P/N 1052497 or equivalent) or lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB
Engine Oil | The engine requires a special oil meeting GM Specification 4718M. Oils meeting this specification may be identified as synthetic, and should also be identified with the American Petroleum Institute (API) Certified for Gasoline Engines STARBURST symbol. However, not all Synthetic API oils with the STARBURST symbol will meet this GM Specification. Look for and use ONLY an oil that meets GM Specification 4718M. For information on the proper oil viscosity, refer to Engine Oil Viscosity under Explanation of Scheduled Services .
Manual Transaxle | Synchromesh Transmission Fluid (GM P/N 12345349)
Hood Latch, Pivots, and Spring Anchor | Lubriplate Lubricant aerosol (GM P/N 12346293 or equivalent) or a lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB
Hood Release Pawl | Lubriplate Lubricant aerosol (GM P/N 12346293 or equivalent) or a lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB
Hydraulic Brake System | Delco Supreme 11® Brake Fluid (GM P/N 12377967) or equivalent DOT-3 brake fluid
Hydraulic Clutch System | Hydraulic Clutch Fluid (GM P/N 12345347 or equivalent)
Key Lock Cylinders | Multi-Purpose Lubricant, Superlube® (GM P/N 12346241 or equivalent)
Parking Brake Cable Guides, Underbody Contact Points and Linkage | Chassis lubricant (GM P/N 1052497) or lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB
Power Steering System | GM Hydraulic Power Steering Fluid (GM P/N 1052884 - 1 pint, 1050017 - 1 quart, or equivalent)
Weatherstrip Conditioning | Dielectric Silicone Grease (GM P/N 12345579 or equivalent)
Windshield Washer Solvent | GM Optikleen® Washer Solvent (GM P/N 1051515 or equivalent)
Automatic Transaxle Shift Linkage | Engine Oil