For 1990-2009 cars

# FUSE IDENTIFICATION LABEL SERVICE INFORMATION

#### SUBJECT: FUSE IDENTIFICATION LABEL SERVICE INFORMATION

#### VEHICLES AFFECTED: 1991 H MODEL

#### CONDITION:

--------- Some early built 1991 "H" Models may have been assembled with a blank fuse identification label. The label is located on the back of the light switch panel to the left of the steering column.

#### CORRECTION:

---------- Install Part Number 25602154 replacement label directly over the blank label.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.