For 1990-2009 cars

### Removal Procedure

Important: The wiper blade element must be replaced if removed from the wiper blade.

1. Remove the wiper blade from the wiper arm. Refer to Windshield Wiper Blade Replacement .
2. Remove the wiper blade element by pulling out through the wiper blade claws.

### Installation Procedure

1. Install the wiper blade element into the wiper blade by sliding the wiper blade element through the wiper blade claws until the claw is locked into the notches in the wiper blade element.

Important: Be sure the wiper blade element is secure in all the claw sets and that the element moves back and forth freely as the wiper blade flexes.

2. Install the wiper blade onto the wiper arm. Refer to Windshield Wiper Blade Replacement .
3. Operate the wipers and check for proper operation.