For 1990-2009 cars

# DELCO GENERATOR EXCHANGE PROGRAM

#### VEHICLES AFFECTED: All 1986 Models with CS-130 or CS-144 Generators

For 1986 some General motors vehicles will use CS-13o or CS-144 model generators. To aid in the analysis of field parts, Delco Remy has instituted an Exchange Only Program which will be handled through the normal parts channels.

Failure to return the suspect generator to the Parts Department will result in a core charge.

The following charts list each generator application.

1986 CS-130 GENERATOR APPLICATION

CARLINE/ REMANUFACTURED TRUCKLINE ENGINE GENERATOR MODEL DIVISION PART NUMBER --------- ------ --------------- -------- ----------- 'F' 2.5L 1105612-IOOA Chevrolet, Pontiac 10497106 'M','S','T' TRUCK

'F' 2.5L 1105662-85A Chevrolet, Pontiac 10497112 'M' TRUCK

'S','T' 2.8L 1105663-85A TRUCK 10497113

'M' 4.3L 1105664-85A TRUCK 10497114

'M' 4.3L 1105665-100A TRUCK 10497115

'N' 2.5L 1105670-IOOA Pontiac,Oldsmobile,Buick 10497119

'N' 2.5L 1105669-85A Pontiac,Oldsmobile,Buick 10497118

'N' 3.OL 1105672-IOOA Pontiac,Oldsmobile,Buick 10497121

'N' 3.OL 1105671-85A Pontiac,Oldsmobile,Buick 10497120

'Y' 5.7L 1105678-105A Chevrolet 10497122

'A' 3.8L 1101158-1000A Oldsmobile, Buick 10497145

'A' 3.8L 1101146-85A Oldsmobile, Buick 10497144

1986 CS-144 GENERATOR APPLICATION

REMANUFACTURED CARLINE ENGINE GENERATOR MODEL DIVISION PART NUMBER

'H' 3.OL 1105626-120A Oldsmobile, Buick 10497110 'H' 3.OL 1105625-108A Oldsmobile, Buick 10456332 * 'A','H','E' 3.8L 1105616-120A Oldsmobile, Buick 10497108 'A','H','E' 3.8L 1105615-108A Pontiac,Oldsmobile,Buick 10456319 * 'G' 3.8L 1105685-120A Buick 10497176 'C','E','K' 4.lL 1105657-120A Cadillac 10497111

* NEW SERVICE PART NUMBERS RELEASED FOR 108 AMP APPLICATION TO CORRECT AN AIRBORNE MAGNETIC FIELD WHINE ON SOME 1986 "A" and "H" MODELS.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.