For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Computer Command Ride (CCR) Module | Left hand front of the passenger compartment, below the left hand front seat | Suspension Controls Component Views | Suspension Controls Connector End Views
Data Link Connector (DLC) | Under the left hand of the instrument panel, on the instrument panel sound insulator | Data Link Communications Component Views in Wiring Systems | Data Link Communications Connector End Views in Wiring Systems
IP Fuse Block | Under the left hand of the instrument panel, on the left hand instrument panel sound insulator | Power and Grounding Component Views in Wirings Systems | Power and Grounding Connector End Views in Wiring Systems
Lateral Acceleration Switch | Left hand front of the passenger compartment, below the left hand front seat | Suspension Controls Component Views | --
Powertrain Control Module (PCM) | Left hand front of the engine compartment, near the air cleaner housing | Engine Controls Component Views in Engine Controls | Powertrain Control Module Connector End Views in Engine Controls
Shift Select Switch C2 | In the console, under the shifter | -- | --
C101 (66 cavities) | Body harness to the engine harness, right hand rear of the engine compartment near the strut tower | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200 (116 cavities) | Body harness to the instrument panel harness, under the center of the instrument panel | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G105 | Right hand front of the engine compartment, near the battery | Power and Grounding Component Views in Wiring Systems | --
P100 | Left hand rear of the engine compartment, near the left hand front strut tower | Harness Routing Views in Wiring Systems | --
P101 | Right hand rear of the engine compartment, near the right hand strut tower | Harness Routing Views in Wiring Systems | --
S246 | In the body harness, approx 8 cm from the interior lamp control module breakout | Harness Routing Views in Wiring Systems | --
S249 (Pontiac) | In the instrument panel harness, approx 3.5 cm from the instrument cluster C1 breakout | Harness Routing Views in Wiring Systems | --
S262 | In the body harness, approx 27.5 cm from P100 | Harness Routing Views in Wiring Systems | --
S270 | In the body harness, approx 8 cm from edge of the right hand instrument panel harness channel end | Harness Routing Views in Wiring Systems | --
S292 | In the body harness, approx 62.5 cm from top edge of the left hand kick wall channel | Harness Routing Views in Wiring Systems | --
SP215 | Under the right hand of the instrument panel, near the instrument panel junction block | Harness Routing Views in Wiring Systems | --