For 1990-2009 cars

Table 1: | Lateral Accelerometer
Table 2: | LH Front Strut Actuator
Table 3: | LH Rear Strut Actuator
Table 4: | RH Front Strut Actuator
Table 5: | RH Rear Strut Actuator
Table 6: | Shift Select Switch C2 (Pontiac)

#### Electronic Suspension Control (CCR) Module

Connector Part Information |

• | 12045537

• | 32 Way F Micro-Pack 100 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
C1 | - | - | Not Used
C2 | DK BLU | 1308 | CCR Module Lateral Acceleration Signal Output
C3 | PPL/WHT | 1490 | CCR Module Signal - WOT
C4 | - | - | Not Used
C5 | LT GRN | 1435 | CCR Switch Signal (Normal)
C6 | BRN/WHT | 1434 | CCR Signal Switch (Firm)
C7 | DK GRN/WHT | 817 | Vehicle Speed Signal
C8 | - | - | Not Used
C9 | DK GRN | 1437 | CCR LED Feed (Firm)
C10 | PNK | 1438 | CCR LED Feed (Normal)
C11- C12 | - | - | Not Used
C13 | WHT/BLK | 1006 | RH Front Ride Control Strut Motor Feed (Increase)
C14 | YEL | 1014 | RH Rear Ride Control Strut Motor Feed (Increase)
C15 | LT BLU | 1770 | Ride Control Diagnostic Signal
C16 | BRN | 641 | Fused Output (Ign)
D1 | BLK/WHT | 251 | Ground
D2 | LT GRN | 1826 | Ride Control Diagnostic Enable Signal
D3 | DK GRN/WHT | 1016 | RH Rear CCR Strut Position Signal
D4 | BRN/WHT | 1012 | LH Rear CCR Strut Position Signal
D5 | LT BLU | 1008 | RH Front CCR Strut Position Signal
D6 | BRN/WHT | 1004 | LH Front CCR Strut Position Signal
D7 | GRY | 1309 | CCR Module Lateral Acceleration Signal Input
D8 | BRN | 1009 | RH Front Ride Control Strut Motor Feed (Decrease)
D9 | PPL | 1017 | RH Rear Ride Control Strut Motor Feed (Decrease)
D10 | LT GRN | 1005 | LH Front Ride Control Strut Motor Feed (Decrease)
D11 | RED/BLK | 1013 | LH Rear Ride Control Strut Motor Feed (Decrease)
D12 | - | - | Not Used
D13 | RED | 1448 | LH Front Ride Control Strut Motor Feed (Increase)
D14 | RED | 1010 | LH Rear Ride Control Strut Motor Feed (Increase)
D15 | - | - | Not Used
D16 | BLK/WHT | 251 | Ground

#### Lateral Accelerometer

Connector Part Information |

• | 12052635

• | 2-Way F Metri-Pak 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 13018 | Computer Command Ride Module Lateral Acceleration Signal - Output
B | GRA | 1309 | Computer Command Ride Module Lateral Acceleration Signal - Input

#### LH Front Strut Actuator

Connector Part Information |

• | 12129129

• | 3-Way F P25 (MD GRA)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 1448 | Ride Control Strut Motor Feed - Left Front Increase Damping
B | BRN/WHT | 1004 | Computer Command Ride Strut Position Signal - Left Front
C | LT GRN | 1005 | Ride Control Strut Motor Feed - Left Front Decrease Damping

#### LH Rear Strut Actuator

Connector Part Information |

• | 12129129

• | 3-Way F P25 (MD GRA)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 1010 | Ride Control Strut Motor Feed - Left Rear Increase Damping
B | BRN/WHT | 1012 | Computer Command Ride Strut Position Signal - Left Rear
C | RED/BLK | 1013 | Ride Control Strut Motor Feed - Left Rear Decrease Damping

#### RH Front Strut Actuator

Connector Part Information |

• | 12129129

• | 3-Way F P25 (MD GRA)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WHT/ BLK | 1006 | Ride Control Strut Motor Feed - Right Front Increase Damping
B | LT BLU | 1008 | Computer Command Ride Strut Position Signal - Right Front
C | BRN | 1009 | Ride Control Strut Motor Feed - Right Front Decrease Damping

#### RH Rear Strut Actuator

Connector Part Information |

• | 12129129

• | 3-Way F P25 (MD GRA)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 1014 | Ride Control Strut Motor Feed - Right Rear Increase Damping
B | DK GRN/WHT | 1016 | Computer Command Ride Strut Position Signal - Right Rear
C | PPL | 1017 | Ride Control Strut Motor Feed - Right Rear Decrease Damping

#### Shift Select Switch Connector C1 (Pontiac)

Connector Part Information |

• | 12047886

• | 7-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 1141 | Fused Output - IGN3
B | BRN/WHT | 1571 | Traction Control Switch Signal
C | BLK/WHT | 251 | Ground
D | DK BLU | 1660 | Tracton Control Indicator Lamp Driver Module Output
E | GRY | 8 | Instrument Panel Lamp Feed
F | BLK | 1250 | Ground
G | LT BLU | 553 | Transmission Shift Select Switch Output - Performance
H | BLK | 808 | Sensor Ground

#### Shift Select Switch C2 (Pontiac)

Connector Part Information |

• | 12047785

• | 4-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 1438 | Computer Command Ride LED Feed - Normal
B | DK GRN | 1437 | Computer Command Ride LED Feed - Firm
C | LT GRN | 1435 | Computer Command Ride Switch Signal - Normal
D | BRN/WHT | 1434 | Computer Command Ride Switch Signal - Firm