For 1990-2009 cars

#### High Speed Engine Cooling Fan Relay

Connector Part Information |

• | 12129716

• | 4-Way F Metri-Pack, Flex-Lock, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
30 | RED | 742 | Fused Output - Battery
85 | BRN | 241 | Fused Output IGN3
86 | DK BLU | 473 | Cooling Fan Relay Output - Coil - Secondary
87 | GRY | 532 | Cooling Fan Motor Feed - Secondary

#### LH Engine Cooling Fan Motor

Connector Part Information |

• | 12124685

• | 3-Way F Metri-Pack 630 Series, Sealed (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 409 | Cooling Fan Motor Feed
B | GRY | 532 | Cooling Fan Motor Feed - Secondary
C | BLK | 1150 | Ground

#### Low Speed Engine Cooling Fan Relay

Connector Part Information |

• | 12129716

• | 4-Way F Metri-Pack 280 Series, Flex Lock, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
30 | RED | 742 | Fused Output - Battery
85 | BRN | 241 | Fused Output - IGN3
86 | DK GRN | 335 | Cooling Fan Relay Output - Coil
87 | LT BLU | 409 | Cooling Fan Motor Feed

#### RH Engine Cooling Fan Motor

Connector Part Information |

• | 12103172

• | 2-Way F Metri-Pack 630 Series, Sealed (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1150 | Ground
B | LT BLU | 409 | Cooling Fan Motor Feed