For 1990-2009 cars

# SMU - SECTION 6E3 - DRIVEABILITY & EMISSION

REVISION: 05/26/95

THIS BULLETIN IS BEING REVISED TO ADD THE 1995 OLDSMOBILE NINETY EIGHT. PLEASE DISCARD CORPORATE BULLETIN NUMBER 51-65-30 (SECTION 6E- ENGINE FUEL AND EMISSIONS). **********************************************************************

#### SUBJECT: SERVICE MANUAL UPDATE-SECTION 6E3-DRIVEABILITY AND EMISSIONS REVISED DTC CHART P1200

#### MODELS: 1995 BUICK PARK AVENUE, RIVIERA 1995 OLDSMOBILE EIGHTY EIGHT, NINETY EIGHT 1995 PONTIAC BONNEVILLE WITH 3.8L ENGINE (VIN K-RPO L36)

THIS BULLETIN CORRECTS THE DTC NUMBER FOR INJECTOR CIRCUIT FAULT IN THE SERVICE MANUAL, SECTION 6E3. P1200, INJECTOR CIRCUIT FAULT, WAS INCORRECTLY IDENTIFIED AS DTC P0200 IN THE SERVICE MANUAL. ANY REFERENCE TO DTC P0200 SHOULD BE CHANGED TO DTC P1200.

PAGES AFFECTED IN THE C/H PLATFORM SERVICE MANUAL ARE AS FOLLOWS:

* 6E3-A-2 * 6E3-A-76 * 6E3-A-77 * DRIVEABILITY AND EMISSIONS INDEX-2

PAGES AFFECTED IN THE 3800 (VIN 1) AND (VIN K) G PLATFORM SERVICE MANUAL ARE AS FOLLOWS:

* 6E3-A-1 * 6E3-A-20 * 6E3-A-74 * 6E3-A-75 * DRIVEABILITY AND EMISSIONS INDEX-1

FIGURES: 00 ATTACHMENTS: 00

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.