For 1990-2009 cars

# INFORMATION ON DEPLOYMENT OF SIR DUAL AIR BAGS

REVISION: 02/18/94

#### BULLETIN REVISED TO ADD 1992 MODEL YEAR TO THE TITLE

#### SUBJECT: INFORMATION ON DEPLOYMENT OF SIR DUAL AIR BAGS

#### MODELS: 1994 BUICK ROADMASTER, LASABRE AND PARK AVENUE 1993-94 CADILLAC BROUGHAM, ELDORADO AND SEVILLE 1994 CADILLAC CONCOURS AND DEVILLE 1993-94 CHEVROLET CAMARO 1994 CHEVROLET CAPRICE AND CORVETTE 1994 GEO PRIZM 1994 OLDSMOBILE EIGHTY EIGHT AND NINETY EIGHT 1993-94 PONTIAC FIREBIRD 1994 PONTIAC GRAND PRIX 1992-94 PONTIAC BONNEVILLE

ON VEHICLES WITH SIR (SUPPLEMENTAL INFLATABLE RESTRAINT) DUAL FRONT AIR BAGS, THE AIR BAGS ARE DESIGNED TO INFLATE IN MODERATE TO SEVERE FRONTAL OR NEAR FRONTAL CRASHES. THE AIR BAGS WILL ONLY INFLATE IF THE VELOCITY OF THE IMPACT IS ABOVE THE DESIGNATED THRESHOLD LEVEL.

IT IS POSSIBLE THAT IN A CRASH, ONLY ONE OF THE TWO AIR BAGS WILL DEPLOY. THIS IS RARE, BUT CAN HAPPEN IN A CRASH JUST SEVERE ENOUGH TO MAKE AN AIR BAG INFLATE.

THIS INFORMATION IS CONTAINED IN THE APPROPRIATE VEHICLE OWNER'S MANUALS STARTING WITH THE 1994 MODEL YEAR.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.