For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Frame Insulator Bolts to the Body Bolts | 90 N·m | 66 lb ft
Front Control Arm Nuts | 190 N·m | 140 lb ft
Front Crosmember to the Body Bolts | 58 N·m | 43 lb ft
Intermediate Shaft to the Steering Gear Stub Shaft - Clamp Bolt | 47 N·m | 35 lb ft
Rear Control Arm Nuts | 123 N·m | 91 lb ft
Retainer Bolts of the Power Steering Cooler Pipe | 7 N·m | 62 lb in
Stabilizer Bar to the Frame Bolts | 47 N·m | 35 lb ft
Stabilizer Link Nut | 17 N·m | 13 lb ft
Tire and the Wheel Nuts | 140 N·m | 100 lb ft
Torque Strut to the Bracket Nut | 40 N·m | 30 lb ft
Transaxle Mount Nuts to the Frame | 40 N·m | 30 lb ft