For 1990-2009 cars

## Water Outlet Installation VIN K

1. Install the thermostat.
2. Install the water outlet gasket.
3. Install the water outlet.
4. Install the water outlet bolts.

Tighten
Tighten the water outlet bolts to 27 N·m (20 lb ft).

## Water Outlet Installation VIN 1

1. Install the thermostat.
2. Install the water outlet gasket.
3. Install the water outlet.
4. Install the water outlet bolts.

Tighten
Tighten the water outlet bolts to 27 N·m (20 lb ft).