For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

• | Close all of the passenger compartment doors.

• | Cycle the ignition switch from RUN to OFF.

The following components operate for approximately 10 minutes or until a passenger compartment door opens.

• | The radio

• | The power windows

• | The sunroof (if equipped)

• | Retained Accessory Power (RAP) Inoperative

• | Retained Accessory Power (RAP) On After Timeout

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.