For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Adjuster Plug Nut | 70 N·m | 50 lb ft
Cylinder End Fittings | 27 N·m | 20 lb ft
Frame to Underbody Bolts | 191 N·m | 141 lb ft
Hexagon Jam Nut | 68 N·m | 50 lb ft
Hexagon Slotted Nut | 47 N·m | 35 lb ft
Inlet/Outlet Hose Retainer Bolts | 6 N·m | 53 lb in
Inner Tie Rod | 100 N·m | 74 lb ft
Intermediate Steering Shaft Pinch Bolt | 47 N·m | lb ft
Outer Hose Retaining Clamp Nuts | 21 N·m | 15 lb ft
Pinion Preload | 1.8 N·m | 16 lb ft
Power Steering Gear Hose Fittings to Pump and Steering Gear | 27 N·m | 20 lb ft
Power Steering Pump Mounting Bolts | 27 N·m | 20 lb ft
Steering Gear Mounting Bolts | 65 N·m | 48 lb ft
Valve End Fitting | 16.9 N·m | 12.6 lb ft