For 1990-2009 cars

#### Model Build Information

Table A
Transmission Model | 8FCB | 8FDB | 8FFB | 8KAB | 8THB
--- | --- | --- | --- | --- | ---
Vehicle Series | C,G | H | C | W Police | W
Engine Displacement | 3.8L | 3.8L | 3.8L | 3.8L | 3.8L
Engine RPO Code | L67 | L67 | L36 | L36 | L36
Engine VIN Code | 1 | 1 | K | K | K
Overall Axle Ratio | 2.93 | 2.93 | 3.05 | 3.29 | 3.29
Final Drive Ratio | 3.29 | 3.29 | 3.05 | 3.29 | 3.29
Drive/Driven Sprocket Teeth | 37/33 | 37/33 | 35/35 | 35/35 | 35/35
VSS Rotor Teeth | 30 | 30 | 30 | 30 | 30
Final Drive Assembly | HD | HD | STD | STD | STD
Output Shaft | LONG | LONG | STD | STD | STD
Torque Converter K-factor | 133 | 133 | 133 | 163 | 163
Converter Clutch | TCC | TCC | TCC | TCC | TCC
Case Side Cover Pan | SSC | SSC | SSC | SSC | SSC
Transmission Vent Assembly | CAP | CAP | CAP | CAP | CAP

• | FP = Fine Pitch

• | HD = Heavy Duty

• | N/A = Not Available

• | SSC = Case Aluminum Structural Side Cover Pan

• | STD = Standard

• | STEEL = Stamped Steel Side Cover Pan

• | VSS = Vehicle Speed Sensor

• | K-factor = Torque converter numeric rating (combines stall speed and torque multiplication ratings)

This chart does not identify all unique build items and this chart may be subject to change.

#### Model Build Information

Table B
Transmission Model | 8TNB | 8TPB | 8YBB | 8YFB | 8XAB
--- | --- | --- | --- | --- | ---
Vehicle Series | W | H | W | H | W
Engine Displacement | 3.8L | 3.8L | 3.5L | 3.8L | 3.8L
Engine RPO Code | L36 | L36 | LX5 | L36 | L67
Engine VIN Code | K | K |  | K | 1
Overall Axle Ratio | 3.05 | 3.05 | 3.05 | 2.86 | 2.93
Final Drive Ratio | 3.05 | 3.05 | 3.05 | 2.86 | 3.29
Drive/Driven Sprocket Teeth | 35/35 | 35/35 | 35/35 | 35/35 | 37/33
VSS Rotor Teeth | 30 | 30 | 30 | 30 | 30
Final Drive Assembly | STD | STD | STD | STD | HD
Output Shaft | STD | STD | STD | STD | LONG
Torque Converter K-factor | 163 | 163 | 164 | 133 | 155
Converter Clutch | TCC | TCC | TCC | TCC | TCC
Case Side Cover Pan | SSC | SSC | SSC | SSC | SSC
Transmission Vent Assembly | CAP | CAP | CAP | CAP | CAP

• | FP = Fine Pitch

• | HD = Heavy Duty

• | N/A = Not Available

• | SSC = Case Aluminum Structural Side Cover Pan

• | STD = Standard

• | STEEL = Stamped Steel Side Cover Pan

• | VSS = Vehicle Speed Sensor

• | K-factor = Torque converter numeric rating (combines stall speed and torque multiplication ratings)

This chart does not identify all unique build items and this chart may be subject to change.