For 1990-2009 cars

Table 1: | Ambient Light Sensor
Table 2: | Ashtray Lamp
Table 3: | Console Storage Lamp
Table 4: | Console Storage Lamp Switch
Table 5: | Daytime Running Lamp (DRL) Resistor
Table 6: | Fog Lamp Switch
Table 7: | Hazard Flasher
Table 8: | Headlamp Switch (Pontiac)
Table 9: | Headlamp Switch (Oldsmobile)
Table 10: | Headlamp Switch (Buick)
Table 11: | High Mounted Stoplamp
Table 12: | Interior Lamp Control Module
Table 13: | Instrument Panel Compartment Lamp
Table 14: | Instrument Panel Compartment Lamp
Table 15: | Instrument Panel Compartment Lamp Switch
Table 16: | Lamp Control Module (LCM) C1 (Buick)
Table 17: | Lamp Control Module (LCM) C2 (Buick)
Table 18: | Lamp Control Module C1 (Oldsmobile/Pontiac)
Table 19: | Lamp Control Module C2 (Oldsmobile/Pontiac)
Table 20: | Lamp Monitor Control Module C1
Table 21: | Lamp Monitor Control Module C2
Table 22: | Lamp Monitor Control Module C3
Table 23: | LH Backup Lamp (Oldsmobile)
Table 24: | LH Cornering Lamp
Table 25: | LH Fog Lamp (Oldsmobile)
Table 26: | LH Fog Lamp (Pontiac)
Table 27: | LH Front Door Courtesy Lamp
Table 28: | LH Front Park Turn Lamp
Table 29: | LH Front Side Marker Lamp
Table 30: | LH High Beam Headlamp
Table 31: | LH High Beam Headlamp (Buick)
Table 32: | LH License Lamp (Oldsmobile/Pontiac)
Table 33: | LH Low Beam Headlamp (Oldsmobile/Pontiac/Buick)
Table 34: | LH Rear Door Courtesy Lamp
Table 35: | LH Rear Side Marker Lamp (Buick/Oldsmobile)
Table 36: | LH/RH Tail/Stop/Turn Lamp
Table 37: | Lamp Dimmer Switch
Table 38: | Perimeter Lighting Relay
Table 39: | Rear Compartment Lamp
Table 40: | Rear Compartment Lid Release Switch
Table 41: | Remote Dimmer Module
Table 42: | RH Cornering Lamp
Table 43: | RH Fog Lamp (Oldsmobile)
Table 44: | RH Fog Lamp (Pontiac)
Table 45: | RH Front Door Courtesy Lamp
Table 46: | RH Front Park/Turn Lamp
Table 47: | RH Front Park/Turn Lamp
Table 48: | RH Front Side Marker Lamp (Buick/Pontiac)
Table 49: | RH High Beam Headlamp
Table 50: | RH License Lamp (Oldsmobile)
Table 51: | RH Low Beam Headlamp
Table 52: | RH Rear Side Marker Lamp (Buick/Oldsmobile)
Table 53: | LH/RH Tail/Stop/Turn Lamp
Table 54: | Turn Signal Flasher
Table 55: | Underhood Lamp

#### Ambient Light Sensor

Connector Part Information |

• | 06288733

• | Lamp Socket Wedge Base W2 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/WHT | 251 | Ground
B | WHT | 278 | Photocell Signal

#### Ashtray Lamp

Connector Part Information |

• | 12047662

• | 2 Way F Metri-Pack Series 150 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 8 | Instrument Panel Lamp Feed
B | BLK | 1250 | Ground

#### Console Storage Lamp

Connector Part Information |

• | 12162222

• | 2 Way F Lamp Socket Wedge Base (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 1732 | BCM Output - 12 Volt Inadvertent Load Control
B | GRY | 157 | Interior Lamp Output

#### Console Storage Lamp Switch

Connector Part Information |

• | 12015197

• | 2 Way F Metri-Pack 280 Series (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 157 | Interior Lamp Output
B | BLK | 1250 | Ground

#### Daytime Running Lamp (DRL) Resistor

Connector Part Information |

• | 12020341

• | 2-Way Metri-Pak 630 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | GRY | 589 | Daytime Running Lamp Resistor Feed
B | TAN | 12E | Low Beam Headlamp Feed

#### Fog Lamp Switch

Connector Part Information |

• | 12064752

• | 6-Way F Metri-Pak 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 9 | Park Lamp Feed
B | BLK | 1250 | Ground
C | ORN/BLK | 434 | Transmission Mounted Neutral Safety Switch Signal
D | BLK | 1576 | Trunk Release Switch Output
E | GRA | 8 | Instrument Panel Lamp Feed
F | YEL | 317 | Fog Lamp Relay Feed Coil

#### Hazard Flasher

Connector Part Information |

• | 02973385

• | 2-Way F 56 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 27 | Hazard Flasher Output
B | ORN | 140 | Fuse Output Battery

#### Headlamp Switch (Pontiac)

Connector Part Information |

• | 12129431

• | 16-Way F Metri-Pak 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | RED | 242 | Fuse Output Battery
B-C | -- | -- | Not Used
D | YEL | 10 | Headlamp Switch Output
E | ORN | 240 | Fuse Output Battery
F | LT BLU | 1785 | Park Lamp Switch Output - Park Lamps OFF
G | BRN | 9 | Park Lamp Feed
H | -- | -- | Not Used
J | GRY | 8 | Instrument Panel Lamp Feed
K | -- | -- | Not Used
L | PPL | 1783 | Twilight Sentinel Delay Signal
M | DK BLU | 1393 | Interior Lamp Relay Output Coil
N | BLK | 1250 | Ground
P | BLK/WHT | 251 | Ground
R | YEL/BLK | 1784 | Twilight Sentinel Enable Signal
S | YEL | 32 | Fuse Output--IP Lamps--Type III Fuse

#### Headlamp Switch (Oldsmobile)

Connector Part Information |

• | 12129432

• | 16-Way F Metri-Pak 280 Series (GRA)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A-B | -- | -- | Not Used
C | YEL | 10 | Headlamp Switch Output
D | RED | 242 | Fuse Output Battery
E | LT BLU | 1785 | Park Lamp Switch Output - Park Lamps OFF
F | LT BLU | 74 | Park Lamp Switch Output
G | ORN | 240 | Fuse Output--Battery--Type III Fuse.
H | -- | -- | Not Used
J | GRA | 8 | Instrument Panel Lamp Feed
K | BLK/WHT | 251 | Ground
L | PPL | 1783 | Twilight Sentinel Delay Signal
M | YEL/BLK | 1784 | Twilight Sentinel Enable Signal
N | BLK | 1250 | Ground
P | -- | -- | Not Used
R | DK GRN | 44 | Instrument Panel Lamps Dimmer Switch Output
S | DK BLU | 1393 | Interior Lamp Relay Output Coil

#### Headlamp Switch (Buick)

Connector Part Information |

• | 12045809

• | 10-Way F Metri-Pak 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK/WHT | 251 | Ground
B | PNK | 1348 | Headlamp ON Indicator Feed
C | DK GRN | 1347 | Park Lamp ON Indicator Feed
D | GRA | 8 | Instrument Panel Lamp Feed
E-F | -- | -- | Not Used
G | GRA/BLK | 308 | Parklamp Switch Signal - Parklamps ON
H | BLK/WHT | 251 | Ground
J | WHT | 103 | Headlamp Switch Signal - Headlamps ON
K | -- | -- | Not Used

#### High Mounted Stoplamp

Connector Part Information |

• | 8911772

• | 2-Way F (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1350 | Ground
B | WHT | 17 | Stoplamp Switch Output (Buick/Oldsmodile
B | LT BLU | 20 | Stoplamp Feed (Pontiac W/UB3)
B | LT BLU/BLK | 1053 | Center High Mounted Stoplamp Feed - Monitored (Pontiac W/U50-UZF)

#### Interior Lamp Control Module

Connector Part Information |

• | 12129077

• | 10-Way F Metri-Pak 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A-C | -- | -- | Not Used
D | DK GRN | 44 | Instrument Panel Lamps Dimmer Switch Output
E | -- | -- | Not Used
F | GRA | 8 | Instrument Panel Lamp Feed
G | -- | -- | Not Used
H | YEL | 32 | Fuse Output - Instrument Panel Lamps
J | -- | -- | Not Used
K | BLK/WHT | 251 | Ground

#### Instrument Panel Compartment Lamp

Connector Part Information |

• | 12124652

• | 2-Way LP SOC WGE (CLR)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 1732 | Electronic Control Unit Output - 12 Volt - Inadvertent Load Control
B | DK BLU/WHT | 148 | Glove Box Lamp Feed

#### Instrument Panel Compartment Lamp

Connector Part Information |

• | 12047662

• | 2-Way F Metri-Pak 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 1732 | Electronic Control Unit Output 12 Volt Inadvertent Load Control
B | BLK | 1250 | Ground

#### Instrument Panel Compartment Lamp Switch

Connector Part Information |

• | 12015197

• | 2-Way F Metri-Pak Series 280 (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1250 | Ground
B | DK BLU/WHT | 148 | Glove Box Lamp Feed

#### Lamp Control Module (LCM) C1 (Buick)

Connector Part Information |

• | 12052854

• | 7 Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 256 | Park Lamp Relay-N.O. Contact
B | LT GRN | 11 | High Beam Headlamp Feed
C | ORN | 240 | Fuse Output -- Battery
D | GRY | 589 | DRL Resistor Feed
E | BLK | 1450 | Ground
F | TAN | 12 | Low Beam Headlamp Feed
G | RED | 242 | Fuse Output-Battery

#### Lamp Control Module (LCM) C2 (Buick)

Connector Part Information |

• | 12110088

• | 24 Way F Micro-Pack 100 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | PNK | 1348 | Headlamp On Indicator Feed
A2 | LT GRN/BLK | 1360 | High Beam Indicator Lamp Ouput
A3 | -- | -- | Not Used
A4 | BLK/WHT | 251 | Ground
A5 | WHT | 278 | Photocell Signal
A6 | PPL | 1783 | Twilight Sentinel Delay Signal
A7 | PNK | 39 | Fuse Output-Ignition 1-Type III Fuse
A8 | LT GRN | 275 | Transmission Mounted Neutral Safety Switch Output-Park
A9 | PPL | 524 | Headlamp Dimmer Switch Output-High Beam
A10-A12 | -- | -- | Not Used
B1 | DK GRN | 1347 | Park Lamp On Indicator Feed
B2 | -- | -- | Not Used
B3 | LT BLU | 1785 | Park Lamp Switch Output-Park Lamps Off
B4 | BLK/WHT | 251 | Ground
B5 | BLK/WHT | 251 | Ground
B6-B9 | -- | -- | Not Used
B10 | WHT | 103 | Headlamp Switch Signal-Headlamps On
B11 | GRY/BLK | 308 | Parklamp Switch Signal-Parklamps On
B12 | BLK/WHT | 624 | Vehicle Anti-Theft System Signal-Headlamp Alarm

#### Lamp Control Module C1 (Oldsmobile/Pontiac)

Connector Part Information |

• | 12110091

• | 6 Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
C | PNK | 3 | Ignition Switch Output - Ignition 1
D | LT BLU | 1346 | Headlamp Relay Output - N.O. Contact (Oldsmobile)
D | YEL | 10 | Headlamp Switch Output (Pontiac)
E | RED | 242 | Fused Output - Battery
F | BRN | 9 | Park Lamp feed
G | GRY | 589 | Daytime Running Lamp Resistor feed
H | ORN | 240 | Fused Output - Battery

#### Lamp Control Module C2 (Oldsmobile/Pontiac)

Connector Part Information |

• | 12084944

• | 16-Way F Micro - Pack 100 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | PPL | 1783 | Twilight Sentinel Delay Signal
A2 | WHT | 278 | Photocell Signal
A3 | LT GRN | 11 | High Beam Headlamp Feed
A4 | DK GRN/WHT | 1317 | Fog Lamp Relay Output - Coil
A5 | BLK/WHT | 251 | Ground
A6 | BLK/WHT | 624 | Vehicle Anti-theft System Signal - Headlamp Alarm
A7 | LT GRN | 275 | Neutral Safety Switch - Park
A8 | -- | -- | Not Used
B1-B5 | -- | -- | Not Used
B6 | BLK/WHT | 251 | Ground
B7 | -- | -- | Not Used
B8 | YEL/BLK | 1784 | Twilight Sentinel Enable Signal

#### Lamp Monitor Control Module C1

Connector Part Information |

• | 12092915

• | 15 Way F ACT 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/WHT | 1312 | Low Beam Headlamp Feed - Monitored
B | DK BLU/WHT | 1315 | Right Front Turn Signal Lamp Feed - Monitored
C | PPL | 1256 | Park Lamp Feed - Tail Lamps - Monitored - Group 1
D | PNK | 1255 | Park Lamp Feed - Side Marker/License - Monitored
E | WHT | 1252 | Park Lamp Feed - Tail Lamps - Monitored - Group 2
F | ORN | 1054 | Stoplamp Feed - Monitored
G | GRY | 1524 | Back-Up Lamp Feed - Monitored
H | DK GRN/WHT | 1335 | Right Rear Turn Signal Lamp Feed - Monitored
J | LT BLU/BLK | 1053 | Center High Mounted Stoplamp Feed - Monitored
K | YEL/BLK | 1334 | Left Rear Turn Signal lamp Feed - Monitored
L | BRN/WHT | 1253 | Right Front Park Lamp Feed - Monitored
M | TAN/WHT | 1254 | Left Front Park Lamp Feed - Monitored
N | -- | -- | Not Used
P | LT BLU/WHT | 1314 | Left Front Turn Signal Lamp Feed - Monitored
R | LT GRN/BLK | 1311 | High Beam Headlamp Feed - Monitored

#### Lamp Monitor Control Module C2

Connector Part Information |

• | 12092914

• | 15-Way F Micro-Pack 280 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN | 11 | High Beam Headlamp Feed
B | LT BLU | 14 | Left Front Turn Signal Lamp Feed
C | -- | -- | Not Used
D | BRN | 9 | Park Lamp Feed
E | -- | -- | Not Used
F | YEL | 18 | Left Rear Stoplamp, Turn Lamp Feed
G | LT BLU | 20 | Pontiac Stop Lamp Feed
H | DK GRN | 19 | Right Rear Stoplamp, Turn Lamp Feed
J | LT GRN | 24 | Back-Up Lamp Feed
K | LT BLU | 20 | Pontiac Stop Lamp Feed
L | -- | -- | Not Used
M | BRN | 9 | Park Lamp Feed
N | -- | -- | Not Used
P | DK BLU | 15 | Right Front Turn Signal Lamp Feed
R | TAN | 12 | Low Beam Headlamp Feed

#### Lamp Monitor Control Module C3

Connector Part Information |

• | 12084945

• | Metri-Pack 100 Series (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | -- | -- | Not Used
A2 | TAN | 1278 | Lamp Monitor Data Request Signal
A3 | -- | -- | Not Used
A4 | WHT | 1279 | Lamp Monitor Data Signal
A5 | -- | -- | Not Used
A6 | BRN | 1141 | Fused Output - IGN
A7 | BLK/WHT | 251 | Ground - Clean
A8 | ORN | 40 | Fused Output - Battery
B1-B8 | -- | -- | Not Used

#### LH Backup Lamp (Oldsmobile)

Connector Part Information |

• | 08917280

• | Type C-2 Axial Bulb Base (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN | 24 | Back Up Lamp Feed
B | -- | -- | Not Used
C | BLK | 1350 | Ground

#### LH Cornering Lamp

Connector Part Information |

• | 12092377

• | 3-Way LPSol WGE BSE (MD GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 57 | Cornering Lamp Feed - Left
B | -- | -- | Not Used
G | BLK | 1150 | Ground

#### LH Fog Lamp (Oldsmobile)

Connector Part Information |

• | 12162000

• | 2-Way M Metri-Pak 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 34 | Fog Lamp Feed
B | BLK | 1250 | Ground

#### LH Fog Lamp (Pontiac)

Connector Part Information |

• | 12020808

• | 2-Way F Metric-Pak Series 280 (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 34 | Fog Lamp Feed
B | BLK | 1250 | Ground

#### LH Front Door Courtesy Lamp

Connector Part Information |

• | 12047663

• | 2-Way M Metri-Pak 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 32 | Fuse Output Instrument Panel Lamps
B | BLK/WHT | 1250 | Ground

#### LH Front Park Turn Lamp

Connector Part Information | LP SOC C2 BSE
--- | ---
Pin | Wire Color | Circuit No. | Function
A | LT BLU | 14 | Turn Signal Lamp Feed - Left Front
B | BRN | 9 | Park Lamp Feed
G | BLK | 1150 | Ground

#### LH Front Side Marker Lamp

Connector Part Information |

• | 12146595

• | Type W-2 Axial (LT GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 9 | Park Lamp Feed
A | TAN/WHT | 1254 | Park Lamp Feed Left Front Monitored (Pontiac W/U50-U2F)
B | LT BLU | 14 | Turn Signal Lamp Feed Left Front
B | LT BLU/WHT | 1314 | Turn Signal Lamp Feed Left Frint Monitored (Pontiac W/U50-U2F

#### LH High Beam Headlamp

Connector Part Information |

• | 12059182

• | 2-Way F Metri-Pak 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN | 11 | Hugh Beam Headlamp Feed (W/UB3)
A | LT GRN/BLK | 1311 | High Beam Headlamp Feed Monitored (W/U50-U2F)
B | BLK | 1150 | Ground

#### LH High Beam Headlamp (Buick)

Connector Part Information |

• | 12059182

• | 2-Way F Metri-Pak 280 Series (MD GRA)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN | 11 | High Beam Headlamp Feed
B | BLK | 1150 | Ground

#### LH License Lamp (Oldsmobile/Pontiac)

Connector Part Information |

• | 12077765

• | Type W-2 Molded On (CRM)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 9 | Park Lamp Feed
B | BLK | 1350 | Ground

#### LH Low Beam Headlamp (Oldsmobile/Pontiac/Buick)

Connector Part Information |

• | 12059180

• | 2-Way Metri-Pak F 280 Series (MD GRA)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN/WHT | 1312 | Low Bean Headlamp Feed Monitored (Pontiac W/U50-U2F
A | TAN | 12 | Low Beam Headlamp Feed
B | BLK | 1150 | Ground

#### LH Rear Door Courtesy Lamp

Connector Part Information |

• | 12059248

• | 2-Way M Metri-Pak Series 150 (MD GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 1732 | Electronic Control Unit Output - 12 Volt - Inadvertent Load Control
B | WHT | 156 | Courtesy Lamp Output

#### LH Rear Side Marker Lamp (Buick/Oldsmobile)

Connector Part Information |

• | 12146595

• | Type W2 Axial (LT GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1350 | Ground (Buick)
A | BRN | 9 | Park Lamp Feed (Oldsmobile)
B | BRN | 9 | Park Lamp Feed (Buick)
B | BLK | 1350 | Ground (Oldsmobile)

#### LH/RH Tail/Stop/Turn Lamp

Connector Part Information |

• | 12047785

• | 4-Way F Metri-Pak 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | YEL | 18 | Stop/Turn Lamp Feed Left Rear
C | BRN | 9 | Park Lamp Feed
D | BLK | 1350 | Ground

#### Lamp Dimmer Switch

Connector Part Information |

• | 12084134

• | 11-Way F Micro-Pak Type III (BRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN/WHT | 1571 | Traction Control System Switch Signal
B | -- | -- | Not Used
C | YEL | 32 | Fuse Output Instrument Panel Lamps
D | -- | -- | Not Used
E | DK BLU | 1393 | Interior Lamp Relay Output Coil
F | BLK | 1250 | Ground
G | BLK/WHT | 251 | Ground
H | GRA | 8 | Instrument Panel Lamp Feed
J | ORN | 40 | Fuse Output Battery
K | DK GRN | 44 | Instrument Panel Lamps Dimmer Switch Output
L | PPL | 1783 | Twilight Sentinel Delay Switch

#### Perimeter Lighting Relay

Connector Part Information |

• | 12110541

• | 6-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A1 | TAN | 1654 | Fuse Output Perimeter Lighting
A2 | LT GRN/WHT | 24 | Back-Up Lamp Feed
B1 | DK GRN | 1655 | Perimeter Lighting Relay Output Coil
B2 | TAN | 1654 | Fuse Output Perimeter Lighting
C1 | ORN | 57 | Cornering Lamp Feed Left
C2 | BLK | 58 | Cornering Lamp Feed Right

#### Rear Compartment Lamp

Connector Part Information |

• | 12047781

• | 3-Way F Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | ORN/ BLK | 737 | Trunk Lamp Output
C | ORN | 1732 | Electronic Control Unit Output 12 Volt Inadvertent Load Control

#### Rear Compartment Lid Release Switch

Connector Part Information |

• | 12015197

• | 2 Way F Metri-Pack 280 Series (BLU)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT BLU | 434 | Transmission Mounted Neutral Safety Switch Signal
B | BLK | 1576 | Trunk Release Switch Output

#### Remote Dimmer Module

Connector Part Information |

• | 12034060

• | 4-Way F Metri - Pack 480 Series (NAT)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | DK GRN | 44 | Instrument Panel Lamps Dimmer Switch Output
C | GRY | 8 | Instrument Panel Lamp Feed
D | YEL | 32 | Fuse Output - Instrument Panel Lamps - Type III Fuse

#### RH Cornering Lamp

Connector Part Information |

• | 12092377

• | Type W-3 Axial (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 58 | Cornering Lamp Feed Right
B | -- | -- | Not Used
G | BLK | 1550 | Ground

#### RH Fog Lamp (Oldsmobile)

Connector Part Information |

• | 12162000

• | 2-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 34 | Fog Lamp Feed
B | BLK | 1450 | Ground

#### RH Fog Lamp (Pontiac)

Connector Part Information |

• | 12020808

• | 2-Way Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PPL | 34 | Fog Lamp Feed
B | BLK | 1450 | Ground

#### RH Front Door Courtesy Lamp

Connector Part Information |

• | 12047663

• | 2-Way M Metri-Pack 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | YEL | 32 | Fuse Output Instrument Panel Lamps
B | BLK | 1450 | Ground

#### RH Front Park/Turn Lamp

Connector Part Information |

• | 8917280

• | Type C-2 Axial (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 15 | Turn Signal Lamp Feed - Right Front
B | BRN | 9 | Park Lamp Feed
G | BLK | 1550 | Ground

#### RH Front Park/Turn Lamp

Connector Part Information |

• | 12160394

• | Type W-3 Right Angle (NAT)

• | 0891780

• | Type C-2 Axial (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | DK BLU | 15 | Turn Signal Lamp Feed - Right Front (B&O-Pont w/UB3)
A | DK BLU/WHT | 1315 | Turn Signal Lamp Feed - Right Front Monitored (Pont w/U50 U2F)
B | BRN | 9 | Park Lamp Feed (B&O-Pont w/UB3)
B | BRN/ WHT | 1253 | Park Lamp Feed - Right Front Monitored (Pont w/ U50 U2F)
G | BLK | 1550 | Ground

#### RH Front Side Marker Lamp (Buick/Pontiac)

Connector Part Information |

• | 12146595

• | Type W-2 Axial (LT GRA)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 9 | Park Lamp Feed (Buick & Pont w/UB3)
A | BRN/ WHT | 1253 | Park Lamp Feed - Right Front Monitored (Pont w/U50 U2F)
B | DK BLU | 15 | Turn Signal Lamp Feed - Right Front (Buick & Pont w/UB3)
B | DK BLU/WHT | 1315 | Turn Signal Lamp Feed - Right Front Monitored (Pont w/ U50 U2F)

#### RH High Beam Headlamp

Connector Part Information |

• | 12059182

• | 2-Way F Metri-Pack 280 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | LT GRN | 11 | High Beam Headlamp Feed (Olds-Pont w/UB3)
A | LT GRN/BLK | 1311 | High Beam Headlamp Feed Monitored (Pont w/U50 U2F)
B | BLK | 1550 | Ground (Pont, Buick)

#### RH License Lamp (Oldsmobile)

Connector Part Information |

• | 12077765

• | Type W-2 Molded On (CRM)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 9 | Park Lamp Feed
B | BLK | 1350 | Ground

#### RH Low Beam Headlamp

Connector Part Information |

• | 12059180

• | 2-Way F Metri-Pack 280 Series (MD GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | TAN | 12 | Low Beam Headlamp Feed
A | TAN/ WHT | 1312 | Low Beam Headlamp Feed - Monitored
B | BLK | 1550 | Ground

#### RH Rear Side Marker Lamp (Buick/Oldsmobile)

Connector Part Information |

• | 12146595

• | LP SOL WGE BSE W2 (LT GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 9 | Park Lamp Feed
B | BLK | 1350 | Ground

#### LH/RH Tail/Stop/Turn Lamp

Connector Part Information |

• | 12047785

• | 4-Way F Metri-Pak 150 Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | -- | -- | Not Used
B | YEL | 18 | Stop/Turn Lamp Feed Left Rear
C | BRN | 9 | Park Lamp Feed
D | BLK | 1350 | Ground

#### Turn Signal Flasher

Connector Part Information |

• | 06288951

• | 2-Way F 56 Series

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 539 | Fuse Output-Ignition 1
B | PPL | 16 | Turn Signal Flasher Output

#### Underhood Lamp

Connector Part Information |

• | 12052635

• | 2-Way F Metric Pack Series 150 (LT GRN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BLK | 1150 | Ground
B | YEL | 32 | Fuse Output - Instrument Panel Lamps