For 1990-2009 cars

## Power Seats System Check AG1/AG2

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Move the LH rear vertical switch up and down. | The rear of the LH seat moves up and down. | Power Seat Does Not Tilt Rearward
2 | Move the LH front vertical switch up and down. | The front of the LH seat moves up and down. | Power Seat Does Not Tilt Forward
3 | Move the LH seat switch forward and back. | The entire LH seat moves forward and back. |

• | Power Seat Does Not Move Forward/Rearward

• | Power Seat Inoperative

4 | For Oldsmobile, move the LH seat recline switch forward and back. | The LH seat back moves forward and back. |

• | Power Seat Does Not Recline

• | Power Seat Inoperative

5 | Move the RH rear vertical switch up and down. | The rear of the RH seat moves up and down. | Power Seat Does Not Tilt Rearward
6 | Move the RH front vertical switch up and down. | The front of the RH seat moves up and down. | Power Seat Does Not Tilt Forward
7 | Move the RH seat switch forward and back. | The entire RH seat moves forward and back. |

• | Power Seat Does Not Move Forward/Rearward

• | Power Seat Inoperative

8 | For Oldsmobile, move the RH seat recline switch forward and back. | The RH seat back moves forward and back. |

• | Power Seat Does Not Recline

• | Power Seat Inoperative

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.

## Power Seats System Check Pontiac w/AL7

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Place the seat select switch in the left position.
2. Briefly press each of the following seat switches:

• | Front vertical: UP

• | Front vertical: DOWN

• | Rear vertical: UP

• | Rear vertical: DOWN

• | Forward/back: FORWARD

• | Forward/back: BACK

• | Recline: FORWARD

• | Recline: BACK

The LH seat moves in the selected direction.

• | Power Seat Select Switch Inoperative

• | Power Seat Inoperative

• | Power Seat Does Not Move Forward/Rearward

• | Power Seat Does Not Tilt Forward

• | Power Seat Does Not Tilt Rearward

• | Power Seat Does Not Recline

2 |

1. Place the seat select switch in the Right position.
2. Briefly press each of the following seat switches:

• | Front vertical: UP

• | Front vertical: DOWN

• | Rear vertical: UP

• | Rear vertical: DOWN

• | Forward/back: FORWARD

• | Forward/back: BACK

• | Recline: FORWARD

• | Recline: BACK

The RH seat moves in the selected direction.

• | Power Seat Select Switch Inoperative

• | Power Seat Inoperative

• | Power Seat Does Not Move Forward/Rearward

• | Power Seat Does Not Tilt Forward

• | Power Seat Does Not Tilt Rearward

• | Power Seat Does Not Recline

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.