For 1990-2009 cars

Name -- | Location | Locator View | Connector End View
--- | --- | --- | ---
Horn Relay | Center rear of the engine compartment, below the right hand underhood fuse block | Horn Component Views in Horns | Horn Connector End Views in Horns
RH IP Fuse Block | Under the right side of the instrument panel, near the rear of the instrument panel compartment | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
LH Horn | At the left front of the engine compartment, near the air cleaner housing | Horn Component Views in Horns | Horn Connector End Views in Horns
C202 (48 cavities) | Body harness to the steering column harness, under the left side of the IP, to the left of the steering column | Harness Routing Views in Wiring Systems | --
G104 | Left front of the engine compartment, near the air cleaner housing | Power and Grounding Component Views in Wiring | --
G105 | Right front of the engine compartment | Power and Grounding Component Views in Wiring | --
P100 | Left rear of the engine compartment, near the left front strut tower | Power and Grounding Component Views in Wiring Systems | --
P101 | Right rear of the engine compartment, near the right front strut tower | Power and Grounding Component Views in Wiring Systems | --
S101 | In the body harness, approximately 15.5 cm (6.1 in) from P101 | Harness Routing Views in Wiring Systems | --
S272 | In the body harness, approximately 12 cm (4.7 in) from the remote function actuator (RFA) module breakout | Harness Routing Views in Wiring Systems | --