For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Press the cigar lighter. | After a few moments, the cigar lighter pops up and the heating element is red hot . | Cigar Lighter Inoperative
2 | Press the rear console cigar lighter (if equipped). | After a few moments, the rear console cigar lighter pops up and the heating element is red hot. | Cigar Lighter Inoperative - Rear
3 | Use the accessory power receptacle (if equipped) to power an electrical accessory . | The electrical accessory operates properly. | Accessory Plug Inoperative - Front Accessory Plug Inoperative - Front
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.