For 1990-2009 cars

DTC | Description | Type | Illuminate ABS/TCS Indicator
--- | --- | --- | ---
C1211 | DTC C1211 ABS Indicator Lamp Circuit Malfunction | ABS | NO
C1214 | DTC C1214 Solenoid Valve Relay Contact or Coil Circuit Open | ABS | ABS/TCS
C1216 | DTC C1216 Brake Control Relay Coil Circuit Open | ABS | ABS/TCS
C1217 | DTC C1217 Pump Motor Relay Contact Circuit Open | ABS | ABS/TCS
C1221 | DTC C1221 LF Wheel Speed Sensor Input Signal is 0 | ABS | ABS/TCS
C1222 | DTC C1222 RF Wheel Speed Sensor Input Signal is 0 | ABS | ABS/TCS
C1223 | DTC C1223 LR Wheel Speed Sensor Input Signal is 0 | ABS | ABS/TCS
C1224 | DTC C1224 RR Wheel Speed Sensor Input Signal is 0 | ABS | ABS/TCS
C1225 | DTC C1225 LF Excessive Wheel Speed Variation | ABS | ABS/TCS
C1226 | DTC C1226 RF Excessive Wheel Speed Variation | ABS | ABS/TCS
C1227 | DTC C1227 LR Excessive Wheel Speed Variation | ABS | ABS/TCS
C1228 | DTC C1228 RR Excessive Wheel Speed Variation | ABS | ABS/TCS
C1232 | DTC C1232 LF Wheel Speed Circuit Open or Shorted | ABS | ABS/TCS
C1233 | DTC C1233 RF Wheel Speed Circuit Open or Shorted | ABS | ABS/TCS
C1234 | DTC C1234 LR Wheel Speed Circuit Open or Shorted | ABS | ABS/TCS
C1235 | DTC C1235 RR Wheel Speed Circuit Open or Shorted | ABS | ABS/TCS
C1236 | DTC C1236 Low System Supply Voltage | ABS | ABS/TCS
C1237 | DTC C1237 High System Supply Voltage | ABS | ABS/TCS
C1238 | DTC C1238 Brake Thermal Model Exceeded | ABS | TCS
C1241 | DTC C1241 Magnasteer Malfunction in Variable Effort Steering | ABS | NO
C1242 | DTC C1242 BPMV Pump Motor Ground Circuit Open | ABS | ABS/TCS
C1243 | DTC C1243 BPMV Pump Motor Stalled | ABS | ABS/TCS
C1255 | DTC C1255 EBCM/EBTCM Internal Malfunction | ABS | ABS/TCS
C1256 | DTC C1256 EBCM/EBTCM Internal Malfunction | ABS | NO
C1261 | DTC C1261 LF Inlet Valve Solenoid Malfunction | ABS | ABS/TCS
C1262 | DTC C1262 LF Outlet Valve Solenoid Malfunction | ABS | ABS/TCS
C1263 | DTC C1263 RF Inlet Valve Solenoid Malfunction | ABS | ABS/TCS
C1264 | DTC C1264 RF Outlet Valve Solenoid Malfunction | ABS | ABS/TCS
C1265 | DTC C1265 LR Inlet Valve Solenoid Malfunction | ABS | ABS/TCS
C1266 | DTC C1266 LR Outlet Valve Solenoid Malfunction | ABS | ABS/TCS
C1267 | DTC C1267 RR Inlet Valve Solenoid Malfunction | ABS | ABS/TCS
C1268 | DTC C1268 RR Outlet Valve Solenoid Malfunction | ABS | ABS/TCS
C1271 | DTC C1271 LF TCS Master Cylinder Isolation Valve Malfunction | ABS | ABS/TCS
C1272 | DTC C1272 LF TCS Prime Valve Malfunction | ABS | ABS/TCS
C1273 | DTC C1273 RF TCS Master Cylinder Isolation Valve Malfunction | ABS | ABS/TCS
C1274 | DTC C1274 RF TCS Prime Valve Malfunction | ABS | ABS/TCS
C1275 | DTC C1275 Serial Data Malfunction | ABS | TCS
C1276 | DTC C1276 Delivered Torque Signal Circuit Malfunction | ABS | TCS
C1277 | DTC C1277 Requested Torque Signal Circuit Malfunction | ABS | TCS
C1278 | DTC C1278 TCS Temporarily Inhibited By PCM | ABS | TCS
C1291 | DTC C1291 Open Brake Lamp Switch Contacts During Deceleration | ABS | TCS
C1293 | DTC C1293 Code C1291 Set in Previous Ignition Cycle | ABS | TCS
C1294 | DTC C1294 Brake Lamp Switch Circuit Always Active | ABS | TCS
C1295 | DTC C1295 Brake Lamp Switch Circuit Open | ABS | TCS