For 1990-2009 cars

## DTC Table Buick, Oldsmobile

Description | DTC
--- | ---
DTC 008 RH Sunload Sensor Circuit Open or Shorted | 008
DTC 010 Outside Temp Sensor Circuit Open/Shorted | 010
DTC 013 Inside Temp Sensor Circuit Open/Shorted | 013
DTC 015 LH Sunload Sensor Circuit Open or Shorted | 015
DTC 034 Pass Control to Programmer Data Loss | 034
DTC 035 Control Assembly to Programmer Data Loss | 035
DTC 036 Pass Control Assy Feedback Out of Range | 036
DTC 036 Pass Control Assy Feedback Out of Range | 036
DTC 038 Loss of Serial Data (UART) | 038
DTC 040 Air Mix Door Motor Circuit Open or Shorted | 040
DTC 041 Pass Air Mix Motor Circuit Open or Shorted | 041
DTC 052 Programmer Loss of Keep Alive Memory (KAM) | 052

## DTC Table Pontiac

Description DTC | DTC
--- | ---
DTC 010 Outside Temp Sensor Circuit Open/Shorted | 010
DTC 013 Inside Temp Sensor Circuit Open/Shorted | 013
DTC 015 LH Sunload Sensor Circuit Open or Shorted | 015
DTC 035 Control Assembly to Programmer Data Loss | 035
DTC 038 Loss of Serial Data (UART) | 038
DTC 040 Air Mix Door Motor Circuit Open or Shorted | 040
DTC 052 Programmer Loss of Keep Alive Memory (KAM) | 052