For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
ABS/TCC Switch | Under the left side of the IP, near the brake pedal | Engine Controls Component Views in Engine Controls -3.8L | Engine Controls Connector End Views in Engine Controls -3.8L
Cruise Control Module | left hand rear of the engine compartment, near the windshield wiper motor | Cruise Control Component Views | Cruise Control Connector End Views
IP Fuse Block | Under the left side of the IP, on the left IP sound insulator | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Powertrain Control Module (PCM) | left front of the engine compartment, near the air cleaner housing | Engine Controls Component Views in Engine Controls -3.8L | Powertrain Control Module Connector End Views in Engine Controls -3.8L
Stoplamp/BTSI Switch | Under the left side of the IP, near the brake pedal | Tilt Wheel/Column Component Views in Steering Wheel and Column - tilt | Tilt Wheel/Column Connector End Views in Steering Wheel and Column - tilt
C101 (66 cavities) | The body harness to the engine harness, in the right rear of the engine compartment, near the strut tower | Harness Routing Views in Wiring Systems | Harness Routing Views in Wiring Systems
C202 (48 cavities) | The body harness to the steering column harness, under the left side of the IP, to the left of the steering column | Harness Routing Views in Wiring Systems | Harness Routing Views in Wiring Systems
G104 | In the left front of the engine compartment, near the air cleaner housing | Power and Grounding Component Views in Wiring Systems | --
P100 | In the left rear of the engine compartment, near the left front strut tower | Harness Routing Views in Wiring Systems | --
P101 | In the right rear of the engine compartment, near the right hand strut tower | Harness Routing Views in Wiring Systems | --
S104 | In the body harness, approximately 25 cm (9.8 in) into the cooling fan relay breakout | Harness Routing Views in Wiring Systems | --
S128 | In the body harness, approximately 6.5 cm (2.6 in) from the engine cooling fan breakout | Harness Routing Views in Wiring Systems | --
S221 | In the body harness, approximately 15.5 cm (6.1 in) from P100 | Harness Routing Views in Wiring Systems | --
S228 | In the body harness, approximately 17.5 cm (6.9 in) from the center IP harness channel breakout | Harness Routing Views in Wiring Systems | --
S230 | In the bnody harness,approx 21.5 cm (8.5in) from the center instrument panel harness channel breakout | Harness Routing Views in Wiring Systems | --
S231 | In the body harness, approximately 17.5 cm (6.9 in) from the center IP harness channel breakout | Harness Routing Views in Wiring Systems | --
S241 | In the body harness, approximately 40 cm (15.7 in) from the interior lamp control module breakout | Harness Routing Views in Wiring Systems | --
S246 | In the body harness, approximately 8 cm (3.1 in) from the interior lamp control module breakout | Harness Routing Views in Wiring Systems | --