For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Data Link Connector (DLC) | Under the left side of the instrument panel, on the instrument panel sound insulator | Data Link Communications Component Views in Data Link Communications | Data Link Communications Connector End Views in Data Link Communications
IP Fuse Block | Under the left side of the instrument panel, on the left instrument panel sound insulator | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
IP Junction Block | Under the right side of the instrument panel, near the rear of the instrument panel compartment | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Park/Neutral Position (PNP) Switch | Left side of the transaxle, below the exhaust gas recirculation valve | Engine Controls Component Views in Engine Controls - 3.8L | Engine Controls Connector End Views in Engine Controls - 3.8L
Remote Function Actuator (RFA) Module | Under the right side of the instrument panel, near the rear of the instrument panel compartment | Keyless Entry Component Views | Keyless Entry Connector End Views
G202 | Left front of the passenger compartment, behind the left kick panel trim plate | Power and Grounding Component Views in Wiring Systems | --
P100 | Left rear of the engine compartment, near the left front strut tower | Harness Routing Views in Wiring Systems | --
S208 | In the body harness, approximately 6 cm (2.3 in) from the center instrument panel harness channel breakout | Harness Routing Views in Wiring Systems | --
S225 | In the body harness, approximately 49.5 cm (19.4 in) from the top edge of the left kick panel channel | Harness Routing Views in Wiring Systems | --
S251 | In the body harness, approximately 10 cm (3.9 in) from the right instrument panel harness channel end | Harness Routing Views in Wiring Systems | --
S278 | In the body harness, approximately 42.5 cm (16.7 in) from the remote function actuator module breakout | Harness Routing Views in Wiring Systems | --
S296 | In the body harness, approximately 13 cm (5.1 in) from the center instrument panel harness channel breakout | Harness Routing Views in Wiring Systems | --