For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Generator | Top RH side of engine | -- | --
I/P Fuse Block | Lower LH side of I/P, behind trim panel | 8A-201-23 Fig. 43 | 11-0
Instrument Panel Cluster | LH side of I/P | -- | 81-0
Ignition Switch | RH side of steering column | 8A-201-22 Fig. 40 | --
Park/Neutral Position (PNP) Switch | Top of LH side of transaxle | 8A-201-9 Fig. 18 | 8A-202-46
PASS-Key® II Decoder Module | Behind RH side of I/P | 8A-201-30 Fig. 55 | 8A-202-5 5
RH MAXI® Fuse Block | RH rear of engine compartment, near P101 | 8A-201-12 Fig. 23 | 10-0
RH I/P Power Distribution Center | Behind RH side of I/P, on multi-use bracket | -- | --
Starter Enable Relay | Behind LH side of I/P, above I/P fuse block | 8A-201-26 Fig. 48 | --
Starter Motor | Front of engine, lower LH | 8A-201-8 Fig. 17 | --
Starter Solenoid | Lower LH front of engine, above starter motor | 8A-201-13 Fig. 25 | --
C101 (66 cavities) | RH rear of engine compartment, near accumulator | 8A-201-7 Fig. 15 | 8A-202-0
C200 (116 cavities) | Below RH side of I/P, near center | 8A-201-25 Fig. 47,47 | 8A-202-11
C202 | LH of I/P, near base of steering column | -- | --
G102 | Front center of engine, near bank #1 knock sensor | 8A-201-13 Fig. 25 | --
G105 | RH front fender, near battery | 8A-201-13 Fig. 9 | --
P100 | Behind LH strut | 8A-201-10 Fig. 19 | --
P101 | RH rear of engine compartment, next to strut tower | -- | --
S217 | Body harn, approx. 20 cm from C202 | 8A-201-26 Fig. 48 | --
S226 | Body harn, approx. 31.5 cm from Data Link Connector (DLC) | 8A-201-26 Fig. 48 | --
S299 (Buick) | I/P harn, approx. 12 cm from Instrument Panel Cluster (IPC) | 8A-201-33 Fig. 63 | --
S299 (Pontiac) | I/P harn, approx. 12 cm from Instrument Panel Cluster (IPC) | 8A-201-33 Fig. 63 | --