FALSE SETTING TROUBLE CODE 44 LEAN CONDITION. Oldsmobile Firenza 1985

For 1990-2009 cars

# FALSE SETTING TROUBLE CODE 44 LEAN CONDITION

#### VEHICLES AFFECTED: 1985 'J' Car with 2.0L Engine (VIN Code P) And Automatic Transmission (MD9) ------------------------------------------

Some 1985 'J' cars with the 2.0L engine and automatic transmission may set the check engine light (Code 44) after extended periods at idle. The setting of a false Code 44 will exhibit the following characteristics:

1. Vehicle must be started and remain in idle for fifty (50) or more seconds (check engine light will then set).

2. Check engine light will go out with movement of the throttle (Code 44 will remain in ECM memory however).

3. Check engine light will not reset again until the vehicle is restarted and remains in idle for fifty (50) or more seconds.

4. Code 44 is more likely to set on a cold or semi-warm engine than a hot engine.

Service PROMS are now available to repair the false setting of Code 44. On vehicles that have set a Code 44, the PROM should be replaced to repair a false code or to eliminate the potential for setting a false Code 44. On vehicles exhibiting characteristics other than those listed above (e.g. the check engine light does not go out with throttle movement) then normal diagnostic procedures for trouble Code 44 should be used to repair the condition.

Applications for service PROMS on vehicles with 2.0L engines and automatic transmissions are:

P/N 16054804 - All body types except convertibles with federal emission (NA5), 2.18 axle (F75) and without air conditioning (C41).

P/N 16054810 - All body types except convertibles with federal emissions (NA5) and either the 3.18 axle with air conditioning (C60) or 3.43 axle (FW9).

All convertibles with federal emissions (NA5).

P/N 16054815 - All body types with California emissions (NB2).

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.