For 1990-2009 cars

The driver information center may be used in order to warn the driver of certain vehicle malfunctions and any required action. Warning messages are displayed by priority, with the higher priority messages displayed first. A list of messages follows. A complete list of messages with an analysis is provided in the diagnostic portion of Instrument Panel, Gauges, and Console. An export ID# accompanies warning messages for non-US vehicles. Warning messages, when active, may be reset or removed from the display by pressing any 1 of the DIC buttons. Warning messages may be superseded by personalization messages if they exist. The following warning messages appear on the DIC:

• | WINDSHIELD WASHER FLUID LOW

• | ENG. COOLANT LOW CHECK LEVEL

• | ENGINE OIL LOW CHECK LEVEL

• | CHANGE ENGINE OIL SOON

• | TRACTION CONTROL SYSTEM ACTIVE

• | CHECK TIRE PRESSURES

• | DOOR AJAR

• | TRUNK AJAR