For 1990-2009 cars

A red BRAKE warning lamp, located in the instrument panel cluster, is turned on when one or more of the following conditions exist:

• | Parking brake applied. The lamp comes on when the parking brake is applied and the ignition switch is on.

• | Low fluid level. The lamp comes on when the fluid level in the master cylinder reservoir becomes to low.

• | During engine cranking. The lamp comes on to indicate that the warning circuit is operating properly.