For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Park/Neutral Position (PNP) Switch | On the left side of the transaxle, below the exhaust gas recirculation valve | Engine Controls Component Views in Engine Controls 3.8L | Engine Controls Connector End Views in Engine Controls 3.8L
Rear Compartment Lid Release Actuator (Buick) | In the center of the rear compartment, on the rear compartment latch | Body Rear End Component Views | Body Rear End Connector End Views
Rear Compartment Lid Release Actuator (Oldsmobile) | In the center of the rear compartment, on the rear compartment latch | Body Rear End Component Views | Body Rear End Connector End Views
Rear Compartment Lid Release Actuator (Pontiac) | In the center of the rear compartment, on the rear compartment latch | Body Rear End Component Views | Body Rear End Connector End Views
Rear Compartment Lid Release Switch (Buick) | Under the left hand of the instrument panel, on the knee bolster | Body Rear End Component Views | Body Rear End Connector End Views
Rear Compartment Lid Release Switch (Oldsmobile) | Left hand of instrument panel, left of the steering column | Body Rear End Component Views | Body Rear End Connector End Views
Rear Compartment Lid Release Switch (Pontiac) | Under the left hand of the instrument panel, on the knee bolster | Body Rear End Component Views | Body Rear End Connector End Views
RH IP Fuse Block | Under the right side of the IP, near the rear of the IP compartment | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Valet Switch (Buick) | Inside the passenger compartment glove box | Body Rear End Component Views | Body Rear End Connector End Views
Valet Switch (Oldsmobile) | Inside the passenger compartment glove box | Body Rear End Component Views | Body Rear End Connector End Views
Valet Switch (Pontiac) | In the rear compartment | Body Rear End Component Views | Body Rear End Connector End Views
C101 (66 cavities) | The body harness to the engine harness, in the right rear of the engine compartment, near the strut tower | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200 (116 cavities) | The body harness to the IP harness, under the center of the IP | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G101 | On the right rear of the engine, below the power steering pump | Power and Grounding Component Views in Wiring Systems | --
G402 (Buick) | In the left side of the rear compartment, on the rear edge of the wheel house | Power and Grounding Component Views in Wiring Systems | --
G402 (Oldsmobile) | Left hand of the rear compartment, on the rear edge of the wheel house | Power and Grounding Component Views in Wiring Systems | --
G402 (Pontiac) | Left hand of the rear compartment, on the rear edge of the wheel house | Power and Grounding Component Views in Wiring Systems | --
P100 | Left hand of the engine compartment, near the left front strut tower | Harness Routing Views in Wiring Systems | --
P405 (Pontiac) | Center rear of luggage compartment lid, near key cylinder | Harness Routing Views in Wiring Systems | --
P408 | Left center of the rear compartment, near the left hand wheel house | Harness Routing Views in Wiring Systems | --
P500 | On the front of the left front door jamb, near the door hinges | Harness Routing Views in Wiring Systems | --
S110 (VIN K) | In the engine harness, approximately 6.5 cm (2.6 in) from the generator breakout | Harness Routing Views in Wiring Systems | --
S110 (VIN 1) | In the engine harness, approximately 6.5 cm (2.6 in) from the generator breakout | Harness Routing Views in Wiring Systems | --
S222 (Oldsmobile) | In the body harness, approximately 15.5 cm (6.1 in) from P100 | Harness Routing Views in Wiring Systems | --
S251 | In the body harness, approximately 10 cm (3.9 in) from the right IP harness channel end | Harness Routing Views in Wiring Systems | --
S273 | In the body harness, approximately 17 cm (6.7 in) into the C101 breakout | Harness Routing Views in Wiring Systems | --
S400 (Buick) | In the body harness, approximately 121.5 cm (47.8 in) from P408 | Harness Routing Views in Wiring Systems | --
S400 (Oldsmobile) | In the body harness, approximately 10 cm (3.9 in) from the G402 breakout | Harness Routing Views in Wiring Systems | --
S400 (Pontiac) | In the body harness, approximately 10 cm (3.9 in) from the G402 breakout | Harness Routing Views in Wiring Systems | --